\begin{table}%TB.1
%\centering
\par
\caption{Main parameters of the simulations with continuously applied
 twisting. $\sigma_{u}$ and $\sigma_{\rho}$ are the smoothing parameters of
 the variables $\rho~u_{x,y,z}$ and $\rho$, respectively. The subscripts
 "in'' and "out'' refer to the "inner region'' of the simulation domain
 with uniform $\nu$ and $\sigma$ and to the rest of the box, respectively.
 $\nu_{\rm in}=0.1$ in all runs.} 
\begin{tabular}{lclllll}
\hline  \hline
 $v_0$ & $\rho_0$ & $y_0$ & $\nu_{\rm out}$ & $1\!-\!\sigma_{u}$ & 
            $1\!-\!\sigma_{\rho,\rm{in}}$ & $1\!-\!\sigma_{\rho,\rm{out}}$\\
\hline 
 0.01  & $B_0^2$       & 0.5 & 0.1--1 & 0.0005 & 0.0005 & 0.0005--0.1 \\ %rsv5
 0.01  & $B_0^2$       & 1.0 & 0.1--1 & 0.0005 & 0.0005 & 0.0005--0.1 \\ %rsv6
 0.01  & $B_0^2$       & 2.0 & 0.1--1 & 0.0005 & 0.0005 & 0.0005--0.1 \\ %rsv7
 0.01  & $|\vec{B}_0|$ & 1.0 & 0.1--1 & 0.0005 & 0.0005 & 0.0005--0.1 \\ %rsv8
 0.01  & $1$           & 1.0 & 0.1--1 & 0.0005 & 0.0005 & 0.0005--0.1 \\ %rsv4
 0.001 & $B_0^2$       & 1.0 & 0.1    & 0.0005 & 0.0005 & 0.0005--0.01\\ %rsv12
 0.001 & $|\vec{B}_0|$ & 1.0 & 0.1    & 0.0001 & 0.0001 & 0.0001      \\ 
\hline  
\end{tabular}
\label{Tab1}
\end{table}