\begin{table}%t4
\par
\caption{Identifiers, positions, peak flux and integrated flux densities for BRC sources
detected at 13 or 20 cm. 3$\sigma$ upper limits for non-detections are indicated.\label{tbl:20/13sources}}
%\centerline
{\begin{tabular}{lccccccl}\hline\hline
	&  &  		 	 & \multicolumn{2}{c}{Peak flux} (mJy/beam)   &
	\multicolumn{2}{c}{Integrated flux} (mJy)   \\ 
Source ID	&  $\alpha$(2000)	 & 	$\delta$(2000)		& 13 cm 	&
20 cm & 13 cm & 20 cm & Type\\\hline 
\object{SFO 47a} & 07:32:10.0 & --19:28:48&	11.7 &	      14.4      & 15.0 & 24.9 & 4\\
\object{SFO 47b} & 07:31:49.0 & --19:24:38&	28.8 &		13.5	& 93.8& 186 & 4\\
\object{SFO 49a} &  07:36:02.5 & --18:53:16 &  242& 	316	&274 & 357 & 4	\\
\object{SFO 49b} & 07:35:34.5 & --18:45:32 &  194& 	294.2	& 463 & 568  & 4 \\
\object{SFO 56} &  08:42:57.0 & --40:00:26 & $<$3.6	&
5.2$^a$	& $<$3.6 &
5.2$^a$ & 4 \\
\object{SFO 58a} &  08:45:15.8 & --41:13:33 &		 2.7  &	$<$1.0 	& 2.7 & $<$1.0 & 4 \\
\object{SFO 58b} &  08:45:19.5 & --41:15:13 &		 6.9  &	$<$1.0 	& 8.7 & $<$1.0 &  1 \\
\object{SFO 59} &  08:58:9.1& --47:21:51 &      3100	&	$<$305	& 10400 & $<$305 & 3 \\ 
\object{SFO 64} &  11:12:13.7 & --58:46:45& 	14.4	&	45.6	& 117 & 236 & 1\\
\object{SFO 69} &  11:41:04.9 & --63:22:05& 	25.4	&	$<$15.0	& 133 & $<$15.0 & 4\\
\object{SFO 74}&   14:19:40.9 & --61:25:17&	9.9	&	25.0	& 26.3 & 37.3  & 3\\
\object{SFO 75}&   15:55:43.4 & --54:39:07&	115.0	&	443	& 247 & 479 & 1
\\
\object{SFO 82a}&  16:47:22.1 & --41:13:06& 	3.0$^a$	&	12.3	& 3.0$^a$& 36.7 & 1 \\
\object{SFO 82b}&  16:47:19.4 & --41:15:43&	5.1	&	23.2	& 6.7 & 63.6 & 1	\\
\object{SFO 84} &  	16:53:51.9 & --40:08:09&	
\ldots $^b$	&	11.7	&
\ldots $^b$ & 28.6 & 1 \\
\object{SFO 85a} & 16:59:04.0&  --42:41:46& 40.3$^b$ & $<$201 & 40.3$^a$ & $<$201 &  3\\
\object{SFO 85b} & 16:59:12.0&  --42:43:15& 67.4 & $<$201 & 97.2 & $<$201 &  4\\
\object{SFO 89}&         18:09:48.9 & --24:04:56 & 		63.2	&	102	& 28.6 &
369 & 1\\
\hline
\end{tabular}}
\smallskip
$^a$ {Source is unresolved at this wavelength}\\
$^b$ {In the cleaned 13~cm image SFO~84 lies in an area affected by a 
striping artefact caused by the cleaning process. It is not possible to set a
sensible flux limit for this source at 13~cm.}
\end{table}