\begin{table}%t3
\caption{Pop.~II.5 models using the $M = 35~M_\odot$ SN~yields of
\cite{chl:2002}. The mass cut has been found by inter- or extrapolating
between SN~models with different ${M_{\rm SN}({\rm Ni})}/{M_\odot}$ 
to obtain the correct ${\rm [C/Fe]}$. ${M({\rm prim})}/{M({\rm
SN})}$ is the mixing proportion between primordial and SN~matter,
needed to reach (approximately) the observed ${\rm [Fe/H]}$-value.
The various parameters of the models start at Col.~5 (age).
Evolutionary models that could represent the
objects are marked by the following labels:
E-RGB: on RGB, but before bump; 
B-RGB: at bump; AB-RGB: after bump; L-RGB: close to tip; E-AGB: on
early AGB, after 2nd dredge-up; L-AGB: immediately before
thermal pulses commence; TP-AGB: thermal pulse phase on AGB.
The last two lines refer to models for CS~22943-037, for which we have
used alternative SN-yields from a~$15~\msun$ model by \citealt{umno:2002} (see
text).} \label{t:3} 
\par
%\centering
\par
\begin{tabular}{cccccccccccccr} 
\hline \hline
\noalign{\smallskip}
Object & $\frac{M_\star}{M_\odot}$ & $\frac{M({\rm prim})}{M({\rm SN})}$ & 
$\frac{M_{\rm SN}({\rm Ni})}{M_\odot}$ & $\frac{\rm Age}{\rm Gyr}$ &
  ${\rm [Fe/H]}$ &  $T_{\rm eff}$~[K]
& $\log g$ & $\log\frac{L}{L_\odot}$ & {\small ${\rm [C/Fe]}$} & {\small${\rm
[N/Fe]}$} & {\small ${\rm [O/Fe]}$} & $\frac{\rm ^{12}C}{\rm ^{13}C}$\\
\noalign{\smallskip}
\hline
\noalign{\smallskip}
{HE~0107-5240} & 0.81 & 350 & $6\times10^{-5}$ & 13.1 & $-$5.31 & 5026 &
2.3 & 1.8 & 4.0 & 2.9 & 4.0 & 61 & {\small E-RGB} \\[0.5mm]
{CS~22943-037} & 0.79 & 10500 & 0.06 & 13.5 & $-$4.03 & 4880 &
1.5 & 2.5 & 1.2
& $-$1.8 & 1.2 & 340 & {\small AB-RGB} \\ 
& & & & 13.6 & $-$4.02 & 4800 & 1.2 & 2.8 & 1.1 & 1.1 &
1.2 & 56 & \small{E-AGB} \\[0.5mm]
{CS~29498-043} & 0.79 & 1170 & 0.1 & 13.7 & $-$3.77 & 4380 &
0.7 & 3.2 & 1.9 & 0.1 & 1.9 & 97 & {\small L-RGB}\\ 
& & & & 13.8 & $-$3.77 & 4400 & 0.6 & 3.2 & 1.8 & 1.9 &
1.9 & 43 & {\small L-AGB} \\
& & & & 13.8 & $-$3.77 & 4400 & 0.6 & 3.2 & 1.8 & 2.0 & 1.9 &
43 & {\small TP-AGB}\\[0.5mm]
{CS~22957-027} & 0.85 & 84 & 0.003 & 13.5 & $-$3.12 & 4800 &
2.4 & 1.7 & 2.4 & 1.7 & 2.4 & 55 & {\small B-RGB}\\[0.5mm]
{CS 22892-052} & 0.795 & 1230 & 0.075 & 13.4 & $-$2.99 & 4790 & 1.5 &
2.5 & 1.1 & $-$0.6 & 1.1 & 94 & {\small AB-RGB} \\ 
& & & & 13.5 & $-$2.99 & 4740 & 1.1 & 2.8 & 1.0 & 0.9 & 1.1
& 33 & {\small E-AGB}\\[0.5mm]
{CS~31082-001} & 0.79 & 0.79 & $0.6$ & 13.5 & $-$2.93 & 4850 &
1.5 & 2.5 & 0.2 & $-$2.7 & 0.2 & 280 & {\small AB-RGB} \\ 
\noalign{\smallskip}
\hline 
\noalign{\smallskip}
{CS~22943-037} & 0.79 & 2720 & 0.067 & 13.5 & $-$4.00 & 4920 & 1.5 & 2.5
& 1.2 & 0.6 & 1.1 & 370 & {\small AB-RGB} \\
& & & & 13.6 & $-$4.00 & 4833 & 1.3 & 2.8 & 1.1 & 1.1
& 1.1 & 59 & {\small E-AGB}\\
\noalign{\smallskip}
\hline
\end{tabular}
\end{table}