\begin{table} %T3
%\renewcommand{\arraystretch}{5}
%\centering
\par
\caption{The parameters of the disk: $z_{\rm l}$ is the
shift and $W_{\rm l}=\sqrt{2}\sigma$ is the  Gaussian broadening term
from the disk which is a measure of the random velocity in the
disk, $R_{\rm inn}$ is the inner radius, $R_{\rm out}$ is the
outer radius. $z_{\rm G}$ and $W_{\rm G}$ represent the parameters
of the Gaussian component.}\label{t3}
\begin{minipage}{17.8cm}
\vbox{\tabskip=0pt   \offinterlineskip  \def\podvuci{\noalign{\hrule}}
\def\razmak{\noalign{\vskip.1cm}}     \halign    to    \hsize{\strut#&
#\tabskip=0pt  plus   10pt  minus5pt  &
 \hfil#\hfil&  #&
 \hfil#\hfil&  #&
\hfil#\hfil&  #&
\hfil#\hfil&  #&
 \hfil#\hfil&  #&
\hfil#\hfil&  #&
\hfil#\hfil&  #&
 \hfil#\hfil&  #&  \hfil#&  #
  \tabskip=0pt\cr\podvuci\noalign{\vskip0.05cm}\podvuci\noalign{\vskip0.09cm}
&& Object &&$i$&& $z^{\rm min,max}_{\rm l}$  &&$W^{\rm min,max}_{\rm l}$
(km\,s$^{-1}$) && $R^{\rm min}_{\rm inn}\
(R_{\rm g})$
&&$R^{\rm max}_{\rm out}\ (R_{\rm g})$  && $z^{\rm min,max}_{\rm G}$ && $W_{\rm
G}$
(km\,s$^{-1}$)&&
$p^{\rm min}$&\cr\noalign{\vskip0.09cm}
\podvuci%\razmak\podvuci
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
&& 3C 120 && 8--30 && --300, +300 &&  1050, 1500 && 350 &&  20\,000 && +30, +300
&& 900 $\pm$ 150 &&2.0 &\cr\noalign{\vskip0.25cm}
&& 3C 273 && 12--30$<$ && --30, +300 && 690, 1760 && 400  && 15\,400 && +30, +60
&& 1380 $\pm$ 150&& 2.3 &\cr\noalign{\vskip0.25cm}
&&MRK 1040&& 5--27$<$ && --250, +300  && 800, 1400 && 100&& 18\,000 && 0 $\pm$ 30
&&
500 $\pm$ 200&& 1.3 &\cr\noalign{\vskip0.25cm}
&&MRK 110&& 7--50  &&--320, +300  && 450, 1250  && 400&& 49\,000 && +150 $\pm$ 30
&&
960 $\pm$ 50&&1.7 &\cr\noalign{\vskip0.25cm}
&&MRK 141 &&12--33 && --630, --450 && 700, 1500 && 300 && 10\,000  && +200, +300
&& 1620 $\pm$ 100&&2.1 &\cr\noalign{\vskip0.25cm}
&&MRK 493 &&5--30$<$ &&  --480, +60 && 360, 560 && 600 && 124\,000  &&
+60 $\pm$ 30 &&
360 $\pm$ 50&&1.8 &\cr\noalign{\vskip0.25cm}
&&MRK 817 && 12--35 && --450, +300&& 850, 1200 && 140 && 14\,000  && 0, +130  &&
1550 $\pm$ 100&&1.8 &\cr\noalign{\vskip0.25cm}
&&MRK 841 &&15--50 &&--750, --150 && 1070, 1800 && 450 && 27\,400  && --300 $\pm$ 30
&&
1500 $\pm$ 100&&2.1 &\cr\noalign{\vskip0.25cm}
&&NGC 3227&&12--34 && --780, --300 && 900, 1550 && 350 && 12\,000  && --300, 300 &&
1500 $\pm$ 100&&2.1 &\cr\noalign{\vskip0.25cm}
&&NGC 4253&&5--25$<$ && --630, --90 && 280, 850 && 500 && 69\,500  && --90, --30  &&
550 $\pm$ 50&&2.0 &\cr\noalign{\vskip0.25cm}
&&PG 1116 &&8--30$<$ &&  --450, 0 && 1100, 1800 && 500 && 15\,800  && 0, +90   &&
1400 $\pm$ 250 &&2.2 &\cr\noalign{\vskip0.25cm}
&&PG 1211 &&8--30 && --660, 0 && 540, 1100 && 600 && 67\,400  && +90 $\pm$ 30  &&
600 $\pm$ 300&& 1.9 &\cr
\podvuci}}
\end{minipage}
\end{table}