\begin{table}%t6
\par
%\centering
\par
\caption{Best fit parameters for different two components spectral models for 1WGA J1713.4--3949 using the MOS and pn data all at once.
The errors are in the range $\Delta \chi^2 < 2.7$ (90\% confidence level) on one parameter. $D_{1}$ is the distance in units of 1 kpc.\label{XPSEC_2}}
\begin{tabular}{clllll}\hline \hline
Two components model & $kT$ (keV)         & $R$ $(D_{1}$ km)  & $L$ $10^{33} \: (D^2_{1} \: {\rm erg} \: {\rm s}^{-1})$ & $\Gamma$   & $N_{{\rm H}}$ ($10^{22}$ cm$^{-2}$) \\ \hline  
Blackbody           & 0.40                &   0.31                          & 0.32           &            & 0.91 \\
$+$                 & (0.38--0.42)         &   (0.28--0.36)                    & (0.28--0.35)     &            & (0.85--0.97) \\
Power law           &                     &                                &               & 4.25         & \\
$\chi^2 = 503$ (473 d.o.f.)  &               &                                &               & (4.03--4.50)  &  \\ \hline 
Blackbody            & $kT_1 = 0.57$      & $R_1 = 0.59$                   & $L_1 = 0.17$  &            & 0.47 \\
$+$                  & (0.52--0.64)        & (0.51--0.69)                     &  (0.14--0.23)  &            & (0.44--0.51) \\
Blackbody            & $kT_2 = 0.32$      & $R_2 = 0.11$                    & $L_2 = 0.44$   &            &   \\ 
$\chi^2 = 490$ (473 d.o.f.) & (0.29--0.34)    & (0.07--0.16)                      & (0.40--0.48)     &            &   \\ \hline
\end{tabular}
\end{table}