\begin{table}%t5
\caption{The best fit results for a model with three {\it xabs}~components fitting all elements but iron, which was fit separately with a~{\it slab}~model (model~C). To fit the full blend we froze the velocity broadening to 200~km~s$^{-1}$ and the outflow velocity to $-$530~km~s$^{-1}$.}
\label{tab:xabs}
%\centering
\par
\begin{tabular}{llll}
\hline  \hline
Comp.             & A             & B           & C     \\
LETGS:            &               &    &    \\
\hline
log $N_{\rm H}$ (m$^{-2}$) & $<$25.9 & $<$25.8 & 24.56 $\pm$ 0.09 \\
log $\xi$ (10$^{-9}$ W m)  & $<$5    & 2.1 $\pm$ 0.6 & 0.8 $\pm$ 0.1\\
LETGS, HEG and MEG:&                  &             &     \\
\hline
log $N_{\rm H}$ (m$^{-2}$) & $<$28   & 25.43 $\pm$ 0.06&24.55 $\pm$ 0.08 \\
log $\xi$ (10$^{-9}$ W m)  & $<$5    & 2.17 $\pm$ 0.05& 0.80 $\pm$ 0.09\\
\hline
\end{tabular}
\end{table}