\begin{table}%t1
%\centering
\par
\caption{Parameters of the jet pulses: the model number, the density of the
pulse in the nozzle $n_{\rm{pulse}}$ in cm$^{-3}$, the velocity of the
pulse in the nozzle $v_{\rm{pulse}}$ in cm~s$^{-1}$, the mass outflow during
the pulse~$\dot M$ in g~s$^{-1}$ and in ${M}_{\odot}$~yr$^{-1}$, and the
kinetic jet luminosity during the pulse in erg~s$^{-1}$. \label{pulses}}
\begin{tabular}{lccccc}
\hline\hline
Model & $n_{\rm{pulse}}$ [cm$^{-3}$] & $v_{\rm{pulse}}$ [cm s$^{-1}$] &
$\dot M$ [g s$^{-1}$] & $\dot M$ [${M}_{\odot}$ yr$^{-1}$] &
$L_{\rm jet}$ [erg s$^{-1}$] \\
\hline
i\arcmin\ & $1.25 \times 10^6$ & $2.0 \times 10^8$ & $2.94 \times 10^{17}$ &
$4.66 \times 10^{-9}$ & $5.88 \times 10^{33}$ \\
iv\arcmin\ & $1.0 \times 10^7$ & $2.0 \times 10^8$ & $2.35 \times 10^{18}$ &
$3.73 \times 10^{-8}$ & $4.70 \times 10^{34}$ \\
\hline
\end{tabular}
\end{table}