\begin{table}%t2
\caption{Relevant parameters of the calibrators used for VINCI
observations of Achernar (continued from
Table~\ref{calib_params1}). The references are the same as in
Table~\ref{calib_params1}. \label{calib_params2}}
\small%\centerline
{
\begin{tabular}{lccc}
\hline\hline
Name & $\epsilon$~Ind~A & $\alpha$~Cet & $\upsilon$~Cet \\
HD number & \object{HD 209100} & \object{HD 18884} & \object{HD 12274} \\
\hline
$m_{\rm V}$ & 4.7 & 2.5 & 4.0 \\
$m_{\rm K}$ & 2.2 & --1.7 & 0.0 \\
Sp. type & K4.5V & M1.5IIIa & K5/M0III \\
$\rm T_{{\rm eff}}$ (K) & 4500 & 3730 & -- \\
$\log g$ & 4.5 & -- & --  \\
$v~\sin i$ (km~s$^{-1}$) & 1 & -- & -- \\
${\theta_{\rm {LD}}}$ (mas)$^{{a}}$ & $1.89 \pm 0.02$ & -- & -- \\
${\theta_{\rm {UD}}}$ (mas)$^{{b}}$ & $1.84 \pm 0.02$  & $11.6 \pm 0.40$ & $5.3 \pm 0.5$\\
 \hline
\end{tabular}}
\smallskip
$^{{a}}$ The angular diameter of $\epsilon$~Ind~A was measured
by Kervella et~al.~(\cite{kervella04b}). 
$^{{b}}$ The uniform disk angular sizes of $\alpha$~Cet and
$\upsilon$~Cet were taken from Dyck et~al.~(\cite{dyck98}) and
Richichi \& Percheron~(\cite{richichi05}), \mbox{respectively}.
\end{table}