\begin{table}%t3
\par
         \caption{Parameters of the components in the VLBI images at 5~GHz. The columns give: (1)
source name and possible classification (CSOc: Compact Symmetric
Object candidate, cj: core-jet); (2) total image intensity
measured with IMEAN at 5~GHz; (3) component identification labled
to Xiang et~al. (\cite{Xiang2002}, \cite{Xiang2005}); (4), (5) peak (per beam) and integral
intensity of component at 5~GHz measured with JMFIT; (6),(7)
major/minor axes (with error $\leq$10\%) and position angle of
component at 5~GHz measured with JMFIT; (8), (9) distance and
position angle relative to the first component; (10) brightness
temperature of component; (11) integrated fractional polarization
in source.}
\par
%\begin{center}
\par
        \begin{tabular}{ccccccccccc}
\par
          \hline
           \hline
\par
            \noalign{\smallskip}
\par
             1&2 &3 &4 & 5& 6 & 7 & 8&9&10&11 \\
\par
Name    & $S_{vlbi}$ & & $S_{\rm p}$    & $S_{\rm int}$ & $\theta_{1}\times\theta_{2}$ & PA  & $d$ && $T$& $m$  \\
\par
class   & [mJy]      &        & [mJy]    & [mJy]          & [mas]    & [$^{\circ}$] & [mas]  &[$^{\circ}$]&
\par
[$10^{7}~{\rm K}^{\circ}$]  & [\%]  \\
\par
            \noalign{\smallskip}
\par
            \hline
\par
            \noalign{\smallskip}
\par
\object{0554$-$026} & $175\pm3$ & AB  & $50.8\pm0.7$ & $114.9\pm2.1$& $7.1\times3.0$& $0.1\pm0.5$ &    0       &    & 2.0 &$\leq$0.4 \\
\par
cj         &           & C   & $17.6\pm0.6$ & $77.3\pm3.4$ & $10.7\times3.9$&$70.4\pm1.3$& $0.4\pm0.1$ &$-69.7\pm4.7$& 0.6&      \\
\par
\object{0914+114} & $116\pm2$ & A   & $27.2\pm0.8$ & $43.0\pm2.0$ & $6.5\times3.3$ &$0.6\pm1.8$  & 0   &  &  0.6&   \\
\par
CSO      &             & B &               &$\leq$$4.3\pm1.9$  &   &   &    &  &&     \\
\par
         &             & tail &            &$20\pm1.3$       &   &   &    &  &&     \\
\par
         &             & C   & $25.2\pm0.8$ & $46.1\pm2.2$ & $6.7\times3.7$ &$4.1\pm2.1$  & $84.3\pm0.1$ &$81.4\pm0.1$ &0.6 &     \\
\par
         &             & D   &            & $\leq$$3.8\pm1.5$  &   &   &    &  &&     \\
\par
\object{1133+432} & $416\pm11$   & A   &           & $290\pm14$ &                  &      &    & &&    \\
\par
CSO      &            & B1  & $44.5\pm0.4$ &$67.4\pm0.9$& $3.2\times2.1$& $35.3\pm0.8$& 0 && &       \\
\par
         &            & B2  & $25.5\pm0.4$ &$53.3\pm1.1$& $3.3\times2.8$& $106.8\pm3.3$& $2.7\pm0.1$&$1.3\pm0.5$& &       \\
\par
\object{1333+589} & $580\pm55$   &N  &$288.5\pm2.4$ &$331.6\pm4.5$& $3.4\times3.2$& $45.1\pm4.8$& 0 &&  &        \\
\par
 CSOc/cj &            & S  &$182.0\pm2.3$ &$225.0\pm4.7$& $3.7\times3.2$& $125.7\pm4.0$ & $12.7\pm0.1$ &$197.5\pm0.5$&&    \\
\par
\object{1433$-$040}&$206\pm10$   &core &$66.5\pm0.3$ & $125.8\pm0.8$& $6.1\times2.8$& $177.8\pm0.2$& 0 &&   & 3.6     \\
\par
 cj      &            & jet &$14.1\pm0.3$ & $67.7\pm1.5$ & $9.6\times4.5$& $17.2\pm0.9$ & $1.4\pm0.2$&$12.4\pm3.5$& & 3.6     \\
\par
\object{1509+054} &        &  E & $76.9\pm1.5$ & $108.3\pm3.3$ & $4.6\times3.7$& $2.3\pm3.5$  & 0  &&2.0 &     \\
\par
 cj      &        &  W & $389.0\pm1.5$& $548.5\pm3.3$& $4.9\times3.5$& $1.5\pm0.5$  & $5.2\pm0.1$&$-89.7\pm0.4$&10.2&    \\
\par
         & $682\pm31$   &  A & $80.8\pm1.5$ & $91.8\pm2.7$ & $3.8\times1.2$& $7.1\pm0.5$  & 0  &&6.5 &     \\
\par
         &            &  B & $317.3\pm1.4$& $464.0\pm3.2$& $4.2\times1.4$& $7.4\pm0.1$  & $5.3\pm0.1$&$-89.2\pm0.1$&25.2& $\leq$0.4      \\
\par
         &            &  C & $38.0\pm1.4$ & $92.8\pm4.5$ & $5.2\times2.0$& $13.6\pm1.3$ & $7.6\pm0.1$&$-81.6\pm0.1$&2.9&      \\
\par
         &            &  D & $27.3\pm1.4$ & $33.2\pm2.8$ & $3.9\times1.3$& $7.6\pm1.6$  & $10.4\pm0.1$&$-97.1\pm0.1$&2.1&     \\
\par
\object{1518+046} & $869\pm9$    &  A & $135.4\pm1.6$& $268.6\pm4.4$& $6.7\times3.9$& $1.9\pm0.9$  &  0 &&  7.0 & $\leq$0.5         \\
\par
CSO/MSO  &            &  B & $49.7\pm1.6$ & $108.9\pm4.8$& $6.7\times4$.3& $4.3\pm2.9$  &  $10.4\pm0.1$&$39.9\pm0.1$&2.6&\\
\par
         &           &  C  & $205.6\pm1.7$& $249.8\pm3.3$& $5.2\times3.1$&$178.9\pm0.6$& $135.8\pm0.1$&$206.7\pm0.1$ &10.5&  $\leq$0.5        \\
\par
         &           &  D  & $97.0\pm1.6$ & $238.0\pm5.2$& $8.0\times4.1$& $23.1\pm0.9$& $133.2\pm0.1$ & $207.0\pm0.1$&4.9&\\
\par
\object{1751+278} & $270\pm10$  &  A  & $163.4\pm0.5$& $243.4\pm1.1$& $5.3\times3.5$& $175.4\pm0.3$& 0  && 7.2 & $\leq$0.4\\
\par
 CSOc/cj &           &  B  & $11.7\pm0.8$ & $20.6\pm2.2$ & $5.8\times3.7$& $7.7\pm6.6$ & $23.3\pm0.2$&$227.5\pm0.1$&0.5 &         \\
\par
\object{1824+271} & $115\pm6$ & A & $48.5\pm0.2$ & $74.3\pm0.5$ & $6.3\times3.9$& $177.3\pm0.4$& 0  &&  &    \\
\par
 CSO     &            &  B & $19.7\pm0.2$ & $31.4\pm0.5$ & $6.1\times4.2$& $175.6\pm1.1$& $21.6\pm0.1$&$-82.6\pm0.1$& &      \\
\par
\object{2121$-$014} & $317\pm9$  & A1 & $99.4\pm0.8$& $154.2\pm1.8$& $6.8\times3.6$& $2.3\pm0.5$ & 0 &&  4.0 &     \\
\par
 CSO     &            & A2 & $8.3\pm0.7$  & $42.0\pm4.3$ & $9.8\times8.3$ &$33.0\pm21.4$&$2.8\pm0.7$&$57.4\pm2.1$& 0.3 &       \\
\par
         &            & B  & $7.4\pm0.8$  & $13.3\pm2.2$ & $6.6\times4.3$ & $0.6\pm11$ &$16.8\pm0.6$&$86.5\pm1.8$   & 0.3 &     \\
\par
         &            & C1 & $33.0\pm0.9$ & $33.7\pm1.6$ & $4.5\times3.6$ & $2.9\pm4.6$&$60.8\pm0.5$&$82.0\pm0.4$&13.4 &     \\
\par
         &            & C2 & $33.4\pm0.8$ & $73.7\pm2.6$ & $9.2\times3.8$ & $1.8\pm1.0$&$61.4\pm0.5$ &$84.4\pm0.4$&13.5&     \\
\par
\object{2322$-$040}& $560\pm15$  & A  & $290.2\pm1.5$& $429.1\pm3.4$& $5.1\times2.7$ &$175.0\pm0.3$ & 0 &&   &         \\
\par
 CSO     &           & tail&$24.4\pm1.5$ & $50.6\pm4.2$ & $7.2\times2.6$ &$3.7\pm2.1$  & $6.7\pm0.2$&$192.5\pm0.2$& &          \\
\par
         &            &  B & $40.7\pm1.5$ & $78.3\pm4.0$ & $6.1\times2.8$ &$157.8\pm1.7$& $37.3\pm0.2$&$176.4\pm0.2$&&    \\
\par
\object{2323+790} & $409\pm13$  &  A1 & $73.6\pm0.3$ & $229.4\pm1.3$& $9.9\times3.7$ &$10.8\pm0.2$  & 0  &&  &         \\
\par
 CSOc/cj &           &  A2 & $110.0\pm0.3$& $123.0\pm0.6$& $4.1\times3.3$ &$172.6\pm0.5$ & $0.2\pm0.1$&$143.4\pm1.2$&&          \\
\par
         &           &  B  & $30.3\pm0.3$ & $45.5\pm0.7$ & $4.8\times3.7$ &$25.0\pm1.7$  & $17.1\pm0.1$ & $-76.8\pm0.1$&&   \\
\par
         &            &  C & $8.7\pm0.3$  & $24.0\pm1.1$ & $7.8\times4.2$ &$9.3\pm2.3$   & $22.5\pm0.2$ & $-77.5\pm0.3$&&   \\
\par
\object{DA193}    &$5272\pm172$ & core & $3415\pm7$&$3943\pm13$&$3.8\times1.5$& $22.7\pm0.1$  & 0 &&  686.5 & 1.0       \\
\par
 cj      &           & jet  & $951\pm7$ &$1300\pm14$&$3.8\times1.8$& $21.2\pm0.3$  & $2.1\pm0.1$&$-48.3\pm0.1$& 191.0& 1.0   \\
\par
\object{OQ208}    &$2656\pm96$ & NE & $1728\pm7$& $2342\pm16$ & $4.7\times2.8$& $3.3\pm0.3$  & 0 &&  56.5 &       \\
\par
 CSO     &          & SW & $173\pm7$ & $236\pm16$  & $4.0\times3.3$& $17.1\pm9.3$ & $6.5\pm0.2$ &$230.2\pm0.2$& 5.7&     \\
\par
\noalign{\smallskip}
\par
            \hline
\par
        \end{tabular}
\par
        %\end{center}
\par
         \label{table:ex004}
\par
   \end{table}