\begin{table}%t2
%\centering
\par
\caption{Parameters of the Galactic single WN stars.
\label{table:parameters}
} 
\small
%%\centering
\par
\begin{tabular}{ l l r r r r r l r c r l r r }
%
\hline\hline %----------------------------------------------------------------- 
\s WR & 
Spectral subtype &
$T_*$ & 
$\log R_{\rm t}$ & 
\multicolumn{1}{c}{$\varv_\infty$} & 
$X_{\rm H}$ & 
$E_{b-\varv}$ & 
Law\a  & 
\DM\ \hspace{5mm} $M_\varv$ &
$R_*$& log~$\dot{M}^\dagger$ & 
log~$L$ & 
$\frac{{\dot M} \varv_{\infty}}{L/c}$ & 
$M$ \\
\par
&      
& 
[kK] & 
$[R_{\odot}]$ & 
\multicolumn{1}{c}{[km~s$^{-1}$]} &
[\%] &
[mag]& 
$R_V$  & 
[mag]\ \ \ [mag] & 
$[R_{\odot}]$ & 
[$M_{\odot}$/yr] &
[$L_{\odot}$] &
&
[$M_{\odot}$] \\
\par
   (1) & (2)           &(3)      & (4)   & \multicolumn{1}{c}{(5)}    
                                             &  (6) & (7)&  (8) & (9) \hspace{0.6cm} (10)
                                                                                   & (11) & (12) & (13)& (14) &(15) \\
\hline %------------------------------------------------------------------------------------------------------------------- 
\s 1    & WN4-s         & 112.2 & 0.3 & 1900 &  0 & 0.67 & S     & 11.3 \r--3.54 & 1.33 & --4.7 & 5.4  &  7.7 & 15 \\
   2    & WN2-w         & 141.3 & 0.5 & 1800 &  0 & 0.44 & C 3.0 & 12.0 \r--2.43 & 0.89 & --5.3 & 5.45 &  1.7 & 16 \\
   3    & WN3h-w        &  89.1 & 1.2 & 2700 & 20 & 0.35 & C 3.4 & 12.4 \l--3.23 & 2.65 & --5.4 & 5.6  &  1.2 & 19 \\
   6    & WN4-s         &  89.1 & 0.3 & 1700 &  0 & 0.12 & S     & 11.3 \r--4.85 & 2.65 & --4.3 & 5.6  & 11.0 & 19 \\
   7    & WN4-s         & 112.2 & 0.3 & 1600 &  0 & 0.53 & S     & 13.4 \l--3.84 & 1.41 & --4.7 & 5.45 &  5.3 & 16 \\
   10   & WN5ha-w       &  63.1 & 1.2 & 1100 & 25 & 0.58 & C 3.1 & 13.3 \r--4.62 & 5.61 & --5.3 & 5.65 &  0.6 & 20 \\
   12\b & WN8h + ?      &  44.7 & 1.0 & 1200 & 27 & 0.80 & C 3.7 & 14.4 \l--7.22 & 21.1 & --4.1 & 6.2  &  2.7 & 44 \\
   16   & WN8h          &  44.7 & 0.9 &  650 & 25 & 0.55 & C 3.4&  13.2 \l--7.22 & 19.9 & --4.3 & 6.15 &  1.2 & 41 \\
   18   & WN4-s         & 112.2 & 0.3 & 1800 &  0 & 0.75 & C 3.6 & 11.5 \l--3.84 & 1.49 & --4.6 & 5.5  &  6.5 & 17 \\
   20   & WN5-w         &  63.1 & 0.9 & 1200 &  0 & 1.28 & S     & 13.8 \l--4.45 & 5.29 & --4.7 & 5.6  &  5.4 & 19 \\
\par
\s 21   & WN5 + O4-6    &  \comp \\
   22\b & WN7h + O9III-V&  44.7 & 1.3 & 1785 & 44 & 0.35 & C 3.8 & 12.55\r --7.85 & 31.5 & --4.2 & 6.55 &  1.8 & 74 \\
   24   & WN6ha-w (WNL) &  50.1 & 1.35& 2160 & 44 & 0.24 & C 3.1 & 12.55\r --7.05 & 19.9 & --4.4 & 6.35 &  1.7 & 54 \\
   25\b & WN6h-w + ? (WNL)&50.1 & 1.5 & 2480 & 53 & 0.63 & C 4.5 & 12.55\r --8.04 & 33.4 & --4.3 & 6.8  &  1.0 & 110\\
   28   & WN6(h)-w      &  50.1 & 1.2 & 1200 & 20 & 1.20 & S     & 13.1 \l --5.06 & 8.89 & --5.0 & 5.65 &  1.3 & 20 \\
   31   & WN4 + O8V     &  \comp \\
   34   & WN5-w         &  63.1 & 0.8 & 1400 &  0 & 1.18 & S     & 14.1 \l --4.45 & 4.72 & --4.7 & 5.5  &  4.0 & 17 \\
   35   & WN6h-w        &  56.2 & 0.9 & 1100 & 22 & 1.15 & S     & 14.2 \l --5.06 & 6.67 & --4.8 & 5.6  &  2.3 & 19 \\
   36   & WN5-s         &  89.1 & 0.2 & 1900 &  0 & 1.00 & S     & 13.9 \l --4.45 & 1.88 & --4.3 & 5.3  & 23.0 & 13 \\
   37   & WN4-s         & 100.0 & 0.4 & 2150 &  0 & 1.63 & S     & 13.2 \l --3.84 & 1.88 & --4.6 & 5.5  &  9.3 & 17 \\
\par
\s 40   & WN8h          &  44.7 & 0.7 & 650  & 23 & 0.40 & C 3.4 & 13.3 \l --7.22 & 17.7 & --4.1 & 6.05 &  2.5 & 35 \\
   44   & WN4-w         &  79.4 & 0.8 & 1400 &  0 & 0.62 & C 3.6 & 13.9 \l --3.84 & 3.15 & --5.0 & 5.55 &  1.9 & 18 \\
   46   & WN3p-w        & 112.2 & 0.8 & 2300 &  0 & 0.30 & F 3.6 & 13.05\r --3.50 & 2.11 & --5.1 & 5.8  &  1.6 & 25 \\
   47   & WN6 + O5V     &  \comp \\
   49   & WN5(h)-w      &  56.2 & 1.0 & 1450 & 25 & 0.80 & S     & 15.0 \l --4.45 & 5.29 & --5.0 & 5.4  &  3.2 & 15 \\
   51   & WN4-w         &  70.8 & 0.9 & 1500 &  0 & 1.40 & S     & 12.9 \l --3.84 & 3.75 & --5.0 & 5.5  &  2.3 & 17 \\
   54   & WN5-w         &  63.1 & 0.9 & 1500 &  0 & 0.82 & S     & 14.1 \l --4.45 & 5.29 & --4.8 & 5.6  &  3.0 & 19 \\
   55   & WN7 (WNE-w)   &  56.2 & 0.8 & 1200 &  0 & 0.65 & C 3.6 & 13.5 \l --5.67 & 8.39 & --4.4 & 5.8  &  3.5 & 25 \\
   61   & WN5-w         &  63.1 & 0.7 & 1400 &  0 & 0.55 & C 2.9 & 14.7 \l --4.45 & 4.21 & --4.7 & 5.4  &  5.9 & 15 \\
   62   & WN6-s         &  70.8 & 0.4 & 1800 &  0 & 1.73 & S     & 12.2 \l --5.06 & 3.54 & --4.2 & 5.45 & 19.0 & 16 \\
\par
\s 63   & WN7 (WNE-w)   &  44.7 & 1.1 & 1700 &  0 & 1.54 & C 3.1 & 12.2 \l --5.67 & 11.2 & --4.6 & 5.65 &  5.3 & 20 \\
   66   & WN8(h)        &  44.7 & 0.9 & 1500 &  5 & 1.00 & S     & 14.8 \l --7.22 & 19.9 & --3.9 & 6.15 &  6.2 & 41 \\
   67   & WN6-w         &  56.2 & 0.8 & 1500 &  0 & 1.05 & S     & 12.6 \r --4.75 & 5.29 & --4.6 & 5.4  &  6.8 & 15 \\
   71   & WN6-w         &  56.2 & 0.9 & 1200 &  - & 0.38 & F 2.5 & 14.0 \l --5.06 & 7.06 & --4.7 & 5.65 &  2.7 & 20 \\
   74   & WN7 (WNE-w)   &  56.2 & 0.7 & 1300 &  0 & 1.50 & S     & 13.0 \r --5.17 & 5.29 & --4.6 & 5.4  &  7.2 & 15 \\
   75   & WN6-s         &  63.1 & 0.6 & 2300 &  0 & 0.93 & S     & 13.0 \r --5.58 & 5.94 & --4.1 & 5.7  & 19.0 & 22 \\
   78   & WN7h          &  50.1 & 1.0 & 1385 & 11 & 0.47 & S     & 11.5 \r --6.82 & 16.7 & --4.2 & 6.2  &  2.6 & 44 \\
   82   & WN7(h)        &  56.2 & 0.7 & 1100 & 20 & 1.00 & S     & 15.5 \l --7.22 & 14.9 & --4.0 & 6.3  &  3.1 & 51 \\
   84   & WN7 (WNE-w)   &  50.1 & 0.9 & 1100 &  0 & 1.45 & S     & 13.3 \l --5.67 & 8.89 & --4.6 & 5.65 &  3.2 & 20 \\
   85   & WN6h-w (WNL)  &  50.1 & 1.1 & 1400 & 40 & 0.82 & C 3.5 & 14.1 \l --7.22 & 21.1 & --4.2 & 6.4  &  1.7 & 59 \\
\par
\s 87   & WN7h          &  44.7 & 1.3 & 1400 & 40 & 1.70 & S     & 12.3 \r --6.68 & 18.8 & --4.6 & 6.1  &  1.4 & 38 \\
   89   & WN8h          &  39.8 & 1.4 & 1600 & 20 & 1.58 & S     & 12.3 \r --7.25 & 26.5 & --4.5 & 6.2  &  1.7 & 44 \\
   91   & WN7  (WNE-s)  &  70.8 & 0.4 & 1700 &  0 & 2.12 & S     & 13.2 \l --5.67 & 5.00 & --4.0 & 5.75 & 14.2 & 23 \\
   94   & WN5-w         &  56.2 & 0.9 & 1300 &  - & 1.49 & C 3.4 & 10.1 \l --4.45 & 6.67 & --4.7 & 5.6  &  3.2 & 19 \\
   100  & WN7  (WNE-s)  &  79.4 & 0.3 & 1600 &  0 & 1.50 & S     & 13.0 \l --5.67 & 3.97 & --4.1 & 5.75 & 12.6 & 23 \\
   105  & WN9h          &  35.5 & 1.1 &  800 & 17 & 2.15 & S     & 11.0 \r --6.90 & 21.1 & --4.5 & 5.8  &  2.2 & 25 \\
   107  & WN8           &  50.1 & 0.8 & 1200 &  - & 1.41 & C 3.7 & 14.6 \l --7.22 & 16.7 & --4.0 & 6.2  &  3.9 & 44 \\
   108  & WN9h          &  39.8 & 1.4 & 1170 & 27 & 1.00 & S     & 13.3 \l --7.22 & 25.1 & --4.6 & 6.15 &  1.0 & 41 \\
   110  & WN5-s         &  70.8 & 0.5 & 2300 &  0 & 0.90 & C 3.5 & 10.6 \l --4.45 & 3.15 & --4.3 & 5.35 & 23.2 & 14 \\
   115  & WN6-w         &  50.1 & 0.9 & 1280 &  0 & 1.50 & S     & 11.5 \r --5.33 & 8.89 & --4.5 & 5.65 &  4.3 & 20 \\
\hline 
\s 116   & WN8h          & 39.8 & 0.8 &  800 & 10 & 1.75 & S     & 13.4 \l --7.22 & 21.1 & --4.0 & 6.0  &  3.9 & 33 \\
   120   & WN7 (WNE-w)   & 50.1 & 0.8 & 1225 &  0 & 1.25 & S     & 12.7 \r --5.52 & 8.39 & --4.4 & 5.6  &  5.7 & 19 \\
   123   & WN8 (WNE-w)   & 44.7 & 0.7 &  970 &  0 & 0.75 & C 2.8 & 15.7 \l --7.22 & 17.7 & --4.0 & 6.05 &  5.5 & 35 \\
   124   & WN8h          & 44.7 & 0.7 &  710 & 13 & 1.08 & C 2.9 & 14.6 \l --7.22 & 16.7 & --4.1 & 6.0  &  3.0 & 33 \\
   127   & WN3 + O9.5V   & \comp \\
   128   & WN4(h)-w      & 70.8 & 1.1 & 2050 & 16 & 0.32 & C 3.6 & 12.9 \l --3.84 & 3.54 & --5.2 & 5.45 &  2.2 & 16 \\
   129   & WN4-w         & 63.1 & 0.9 & 1320 &  0 & 0.85 & S     & 13.6 \l --3.84 & 3.75 & --5.1 & 5.3  &  2.8 & 13 \\
   130   & WN8(h)        & 44.7 & 1.0 & 1000 & 12 & 1.46 & S     & 13.8 \l --7.22 & 22.1 & --4.2 & 6.25 &  1.8 & 47 \\
   131   & WN7h          & 44.7 & 1.3 & 1400 & 20 & 1.15 & S     & 14.9 \l --7.22 & 23.7 & --4.4 & 6.3  &  1.3 & 51 \\
   133   & WN5 + O9I     & \comp \\
\s 134   & WN6-s         & 63.1 & 0.7 & 1700 &  0 & 0.47 & C 3.4 & 11.2 \r --5.07 & 5.29 & --4.4 & 5.6  &  7.8 & 19 \\
   136   & WN6(h)-s      & 70.8 & 0.5 & 1600 & 12 & 0.45 & S     & 10.5 \r --4.69 & 3.34 & --4.5 & 5.4  & 10.9 & 15 \\
   138   & WN5-w + B?    & \comp \\
   139   & WN5 + O6II-V  & \comp \\
   141   & WN5-w + O5V-III& \comp \\
   147   & WN8(h) + B0.5V& 39.8 & 0.9 & 1000 &  5 & 2.85 & S     & 10.4 \l --7.22 & 29.8 & --3.8 & 6.3  &  3.6 & 51 \\
   148\b & WN8h + B3IV/BH& 39.8 & 1.3 & 1000 & 15 & 0.83 & C 3.0 & 14.4 \l --7.22 & 26.5 & --4.5 & 6.2  &  1.0 & 44 \\
   149   & WN5-s         & 63.1 & 0.7 & 1300 &  0 & 1.42 & S     & 13.3 \l --4.45 & 3.97 & --4.7 & 5.35 &  5.2 & 14 \\
   151   & WN4 + O5V     & \comp \\
   152   & WN3(h)-w      & 79.4 & 1.1 & 2000 & 13 & 0.50 & C 3.2 & 12.2 \r --2.65 & 2.23 & --5.5 & 5.25 &  1.7 & 12 \\
\s 155   & WN6 + 09II-Ib & \comp \\
   156   & WN8h          & 39.8 & 1.1 &  660 & 27 & 1.22 & S     & 13.3 \l --7.22 & 23.7 & --4.5 & 6.1  &  0.9 & 38 \\
   157   & WN5-w (+B1II) & \comp \\
   158   & WN7h + Be?    & 44.7 & 1.2 &  900 & 30 & 1.08 & S     & 14.3 \l --7.22 & 25.1 & --4.5 & 6.35 &  0.7 & 54 \\
\hline 
\end{tabular}
\par
\smallskip
\par
 \a\   Column~(8) Applied reddening law: S = Seaton (\cite{Seaton1979}), C = Cardelli et~al. (\cite{Cardelli+al1989}), 
F = Fitzpatrick (\cite{Fitzpatrick1999}); for the last two, the given number is the adopted $R_V$.
\\
 \b\   Binary system in which the non-WR component contributes more than 15\% of the flux in the visual.
\\
  $^\dagger$   Mass-loss rates are for an adopted clumping factor of $D$ = 4.
\end{table}