\begin{table}%t3
\caption {Properties of the CO outflow.}
\label{tco}
%\centerline
{\begin{tabular}{lccccc}
\hline\hline\noalign{\smallskip}
&\multicolumn{1}{c}{$v^{a}$}&
\multicolumn{1}{c}{$M^{b}$}&
\multicolumn{1}{c}{$P^{c}$}&
\multicolumn{1}{c}{$E^{c}$}&
\multicolumn{1}{c}{$\dot P^{c}$}
\\
\multicolumn{1}{c}{Lobe}&
\multicolumn{1}{c}{(\kms)}&
\multicolumn{1}{c}{($10^{-2} M_\odot$)}&
\multicolumn{1}{c}{($M_\odot$ \kms)}&
\multicolumn{1}{c}{($10^{43}$ erg)}&
\multicolumn{1}{c}{($M_\odot ~ \mbox{km s}^{-1}$~yr$^{-1}$)}
\\
\hline\noalign{\smallskip}
Blue &[$-30.5, -13.5$] &8.3  &0.60  &4.78   &$7.5\times10^{-5}$\\
Red$^{d}$ &[$-8.5, -2.5$]    &0.2  &0.01 &0.03  &$2.3\times10^{-6}$ \\
Total &                &8.5  &0.61 &4.81  &$7.7\times10^{-5}$ \\
\hline
\end{tabular}}
\medskip
\par
$^a$~Range of outflow velocities. Momenta and kinetic energies are calculated relative to
the cloud velocity, which is taken to be $V_{\rm LSR}=-11$~\kms. 
$^b$~Assuming an excitation temperature of 24~K. 
$^c$~Velocity not corrected for inclination. 
$^d$~The outflow has only been detected for this velocity range.  
\end{table}