\begin{table}%t2
\caption{Selection cuts optimised for various purposes, as described
in the text. Cuts are applied on MRSW and MRSL, as well as on the distance~($\theta$) from the reconstructed shower position to the source. A~minimum of two telescopes passing the per-telescope cuts, on image amplitude and distance from the centre of the field of view, are also
required. Standard cuts, as well as \emph{hard}, \emph{loose} and
\emph{extended} cuts, as described in the text, are listed.}
\label{tab:selcuts}
%\centering
\small
\begin{tabular}{cccccccc}
\hline\hline
 & & & & & & & \\[-8pt]
Configuration&MRSL&MRSL&MRSW&MRSW &$\theta_{\rm cut}^{2}$ &Image Amp. &Distance\\
             &Min. &Max. &Min. &Max. &Max.          &Min.        &Max.     \\
             &    &    &    &    &(degrees$^{2}$) &(p.e.)     &(\dg)  \\
\hline
Standard     &--2.0&2.0 &--2.0&0.9 &0.0125       &80        &2.0\\
Hard         &--2.0&2.0 &--2.0&0.7 &0.01         &200       &2.0\\
Loose        &--2.0&2.0 &--2.0&1.2 &0.04         &40        &2.0\\
Extended     &--2.0&2.0 &--2.0&0.9 &0.16         &80        &2.0\\
\hline
\end{tabular}
\end{table}