\begin{table}%t5
\caption{Radio properties of HzRGs.}\label{tab:radio}
\small%\centerline
 {
\begin{tabular}{lcccc}
\hline \hline
Source & $D_{\rm ang}$  & $D_{\rm phys}$ & ${\cal L}_{0.1-1}$ & $\tau_{1.4~{\rm GHz}}$ \\
 (1)  & (2)         & (3)            & (4) & (5) \\
\hline
MRC0316-257 & 7.6  & 58  & 45.0 & 0.94\\
MRC0406-244 & 7.3  & 59  & 45.2 & 0.96\\
TXS0828+193 & 12.8 & 103 & 45.4 & 1.7\\
\hline
MRC1138-262 & 11.1 & 92  & 45.2 & 1. \\
\hline
\end{tabular}}
\medskip
For comparison we add MRC1138-262 from \citet{nesvadba06}.  Column (1) -- source name. Column (2) -- maximal projected angular size of the radio source. Column (3) -- maximal projected size in kpc. Column (4) -- integrated luminosity between 0.1 and 1.0~GHz in the rest-frame in erg~s$^{-1}$~cm$^{-2}$, corresponding to $\sim$$0.001{-}0.1 \times$ the kinetic
luminosity. Column (5) -- age of the radio jet for a constant expansion speed of $0.01~c$ in $10^7$~yrs. Angular size distances are taken from \citet{debreuck01}, radio luminosities are based on the VLA~measurements of \citet{carilli97}. 
\end{table}