\begin{table}%t3
\caption{\label{tabprop}Summary of source properties.}
\small%\centerline
 {
 {
\begin{tabular}{lrrrrrrrr}
\hline\hline
Source &  $z$ & $r$ &$(v/c)$ & $(v/c)$ & $a_{L}$ & $P_{10}$ &  $L_j$ & $n_{a}$ \\
    &  & kpc & ($b=0.25$) & ($b=1$) & kpc & $10^{-10}$ dynes cm\mtwo & $10^{44}$
erg s\mone     &
$10^{-3}$ cm\mthree \\
\hline
3C 
239  &       1.790   &       69.5    &$      0.044   \pm     0.008   $&$ 
   0.29    \pm     0.05    $&$     10.0    \pm     0.4     $&$
15.3    \pm     1.8     $&$     242     \pm     86      $&$     0.6 
\pm     0.3     $\\
3C 
322  &       1.681   &       139.4   &$      0.036   \pm     0.006   $&$ 
   0.21    \pm     0.03    $&$     19.6    \pm     1.0
$&$     5.0     \pm     0.6     $&$     250     \pm     89      $&$ 
0.3     \pm     0.1     $\\
3C 
322  &       1.681   &       185.3   &$      0.050   \pm     0.015   $&$ 
   0.31    \pm     0.10    $&$     11.5    \pm     1.2
$&$     11.3    \pm     1.6     $&$     264     \pm     121     $&$ 
0.3     \pm     0.2     $\\
3C 68.2 
&       1.575   &       104.7   &$      0.055   \pm     0.015   $&$ 
0.37    \pm     0.11    $&$     8.2     \pm     1.9
$&$     6.1     \pm     1.2     $&$     80      \pm     43      $&$ 
0.1     \pm     0.1     $\\
3C 68.2 
&       1.575   &       115.8   &$      0.053   \pm     0.009   $&$ 
0.37    \pm     0.07    $&$     9.3     \pm     1.1
$&$     8.9     \pm     1.3     $&$     144     \pm     55      $&$ 
0.2     \pm     0.1     $\\
3C 
437  &       1.480   &       168.4   &$      0.049   \pm     0.004   $&$ 
   0.28    \pm     0.03    $&$     18.1    \pm     1.3
$&$     5.2     \pm     0.6     $&$     294     \pm     98      $&$ 
0.2     \pm     0.1     $\\
3C 
437  &       1.480   &       160.5   &$      0.080   \pm     0.007   $&$ 
   0.54    \pm     0.06    $&$     16.7    \pm     1.3
$&$     9.6     \pm     1.2     $&$     760     \pm     249     $&$ 
0.11    \pm     0.04    $\\
3C 
324  &       1.210   &       35.2    &$      0.038   \pm     0.010   $&$ 
   0.26    \pm     0.07    $&$     7.1     \pm     1.4     $&$
11.5    \pm     2.0     $&$     77      \pm     39      $&$     0.6 
\pm     0.4     $\\
3C 
194  &       1.190   &       50.3    &$      0.023   \pm     0.002   $&$ 
   0.15    \pm     0.02    $&$     7.2     \pm     1.6     $&$
5.5     \pm     1.0     $&$     23      \pm     11      $&$     0.8 
\pm     0.3     $\\
3C 
194  &       1.190   &       79.6    &$      0.025   \pm     0.002   $&$ 
   0.17    \pm     0.02    $&$     8.9     \pm     1.3     $&$
4.8     \pm     0.7     $&$     35      \pm     13      $&$     0.6 
\pm     0.2     $\\
3C 
267  &       1.144   &       175.1   &$      0.032   \pm     0.007   $&$ 
   0.21    \pm     0.05    $&$     8.8     \pm     1.2     $&$
11.2    \pm     1.7     $&$     97      \pm     41      $&$     0.8 
\pm     0.4     $\\
3C 
267  &       1.144   &       165.6   &$      0.029   \pm     0.005   $&$ 
   0.19    \pm     0.03    $&$     10.7    \pm     0.9
$&$     7.9     \pm     1.0     $&$     95      \pm     34      $&$ 
0.7     \pm     0.3     $\\
3C 
356  &       1.079   &       377.1   &$      0.048   \pm     0.012   $&$ 
   0.26    \pm     0.07    $&$     13.6    \pm     2.2
$&$     3.4     \pm     0.5     $&$     105     \pm     49      $&$ 
0.11    \pm     0.07    $\\
3C 
356  &       1.079   &       251.4   &$      0.045   \pm     0.010   $&$ 
   0.28    \pm     0.06    $&$     13.6    \pm     2.2
$&$     6.5     \pm     1.0     $&$     190     \pm     84      $&$ 
0.24    \pm     0.14    $\\
3C 
280  &       0.996   &       49.3    &$      0.027   \pm     0.004   $&$ 
   0.18    \pm     0.03    $&$     7.7     \pm     0.5     $&$
12.0    \pm     1.4     $&$     69      \pm     24      $&$     1.2 
\pm     0.5     $\\
3C 
280  &       0.996   &       60.4    &$      0.014   \pm     0.002   $&$ 
   0.08    \pm     0.01    $&$     7.7     \pm     0.3     $&$
7.7     \pm     0.9     $&$     22      \pm     8       $&$     3.1 
\pm     1.3     $\\
3C 
268.1        &       0.974   &       201.8   &$      0.025   \pm     0.005 
   $&$     0.15    \pm     0.03    $&$     14.5    \pm     0.7
$&$     2.6     \pm     0.3     $&$     48      \pm     17      $&$ 
0.31    \pm     0.15    $\\
3C 
268.1        &       0.974   &       171.6   &$      0.041   \pm     0.007 
   $&$     0.26    \pm     0.05    $&$     13.8    \pm     0.7
$&$     4.1     \pm     0.5     $&$     114     \pm     40      $&$ 
0.18    \pm     0.08    $\\
3C 
289  &       0.967   &       44.5    &$      0.019   \pm     0.003   $&$ 
   0.13    \pm     0.02    $&$     8.9     \pm     0.3     $&$
7.2     \pm     0.8     $&$     38      \pm     12      $&$     1.6 
\pm     0.6     $\\
3C 
289  &       0.967   &       46.1    &$      0.021   \pm     0.003   $&$ 
   0.14    \pm     0.02    $&$     9.7     \pm     0.4     $&$
7.2     \pm     0.8     $&$     50      \pm     16      $&$     1.3 
\pm     0.5     $\\
3C 
325  &       0.860   &       77.7    &$      0.027   \pm     0.005   $&$ 
   0.18    \pm     0.03    $&$     5.2     \pm     1.8     $&$
5.1     \pm     1.3     $&$     14      \pm     8       $&$     0.52 
\pm     0.27    $\\
3C 
325  &       0.860   &       55.0    &$      0.046   \pm     0.010   $&$ 
   0.33    \pm     0.08    $&$     7.0     \pm     1.3     $&$
17.6    \pm     2.8     $&$     144     \pm     63      $&$     0.62 
\pm     0.34    $\\
3C 
265  &       0.811   &       250.0   &$      0.031   \pm     0.005   $&$ 
   0.21    \pm     0.04    $&$     9.5     \pm     1.3     $&$
4.9     \pm     0.7     $&$     48      \pm     19      $&$     0.38 
\pm     0.18    $\\
3C 
265  &       0.811   &       294.3   &$      0.021   \pm     0.004   $&$ 
   0.11    \pm     0.02    $&$     9.5     \pm     1.3     $&$
3.2     \pm     0.5     $&$     21      \pm     9       $&$     0.56 
\pm     0.28    $\\
3C 
247  &       0.749   &       39.5    &$      0.027   \pm     0.005   $&$ 
   0.17    \pm     0.03    $&$     7.8     \pm     0.8     $&$
5.4     \pm     0.7     $&$     31      \pm     12      $&$     0.57 
\pm     0.27    $\\
3C 
247  &       0.749   &       64.7    &$      0.017   \pm     0.003   $&$ 
   0.12    \pm     0.02    $&$     5.8     \pm     0.4     $&$
7.5     \pm     0.9     $&$     15      \pm     5       $&$     1.9 
\pm     0.8     $\\
3C 
55   &       0.720   &       261.7   &$      0.044   \pm     0.009   $&$ 
   0.29    \pm     0.06    $&$     11.6    \pm     1.0     $&$
4.5     \pm     0.6     $&$     95      \pm     35      $&$     0.18 
\pm     0.09    $\\
3C 
55   &       0.720   &       268.0   &$      0.055   \pm     0.011   $&$ 
   0.37    \pm     0.08    $&$     9.5     \pm     1.3     $&$
4.6     \pm     0.7     $&$     82      \pm     32      $&$     0.12 
\pm     0.06    $\\
3C 
337  &       0.630   &       196.1   &$      0.018   \pm     0.005   $&$ 
   0.09    \pm     0.03    $&$     9.7     \pm     0.7     $&$
1.4     \pm     0.2     $&$     8       \pm     3       $&$     0.32 
\pm     0.20    $\\
3C 
337  &       0.630   &       109.5   &$      0.014   \pm     0.001   $&$ 
   0.08    \pm     0.01    $&$     16.5    \pm     0.6
$&$     1.6     \pm     0.2     $&$     22      \pm     7       $&$ 
0.61    \pm     0.22    $\\
3C 
427.1        &       0.572   &       82.8    &$      0.010   \pm     0.002 
   $&$     0.06    \pm     0.01    $&$     13.7    \pm     0.4
$&$     2.7     \pm     0.3     $&$     18      \pm     6       $&$ 
2.1     \pm     0.8     $\\
3C 
427.1        &       0.572   &       75.0    &$      0.011   \pm     0.002 
   $&$     0.08    \pm     0.01    $&$     8.9     \pm     0.6
$&$     4.4     \pm     0.5     $&$     14      \pm     5       $&$ 
2.5     \pm     1.0     $\\
3C 
330  &       0.549   &       205.9   &$      0.031   \pm     0.005   $&$ 
   0.21    \pm     0.04    $&$     10.3    \pm     1.4
$&$     4.0     \pm     0.6     $&$     47      \pm     18      $&$ 
0.3     \pm     0.1     $\\
3C 
330  &       0.549   &       199.7   &$      0.029   \pm     0.005   $&$ 
   0.19    \pm     0.04    $&$     10.3    \pm     0.9
$&$     3.3     \pm     0.4     $&$     36      \pm     13      $&$ 
0.28    \pm     0.13    $\\
3C 
244.1        &       0.430   &       155.9   &$      0.015   \pm     0.001 
   $&$     0.08    \pm     0.01    $&$     8.5     \pm     0.5
$&$     1.4     \pm     0.2     $&$     5       \pm     2       $&$ 
0.49    \pm     0.16    $\\
3C 
244.1        &       0.430   &       141.4   &$      0.024   \pm     0.002 
   $&$     0.16    \pm     0.02    $&$     7.2     \pm     0.5
$&$     3.1     \pm     0.4     $&$     14      \pm     4       $&$ 
0.40    \pm     0.12    $\\
3C 
405  &       0.056   &       63.8    &$      0.009   \pm     0.001   $&$ 
   0.07    \pm     0.01    $&$     10.7    \pm     0.3     $&$
7.4     \pm     0.9     $&$     26      \pm     6       $&$     7.7 
\pm     2.7     $\\
3C 
405  &       0.056   &       72.5    &$      0.009   \pm     0.001   $&$ 
   0.07    \pm     0.01    $&$     10.7    \pm     0.3     $&$
6.1     \pm     0.7     $&$     22      \pm     5       $&$     6.3 
\pm     2.4     $\\
3C 
6.1  &       0.840   &       106.0   &$      0.052   \pm     0.009   $&$ 
   0.25    \pm     0.04    $&$     4.99    \pm     0.07
$&$     8.09    \pm     0.07    $&$     38      \pm     7       $&$ 
0.22    \pm     0.06    $\\
3C 
6.1  &       0.840   &       92.2    &$      0.047   \pm     0.008   $&$ 
   0.18    \pm     0.03    $&$     11.29   \pm     0.03
$&$     3.04    \pm     0.01    $&$     64      \pm     15      $&$ 
0.10    \pm     0.03    $\\
3C 
34   &       0.690   &       170.4   &$      0.045   \pm     0.004   $&$ 
   0.15    \pm     0.01    $&$     13.91   \pm     0.01
$&$     2.01    \pm     0.01    $&$     63      \pm     13      $&$ 
0.07    \pm     0.01    $\\
3C 
34   &       0.690   &       149.9   &$      0.038   \pm     0.002   $&$ 
   0.12    \pm     0.01    $&$     11.28   \pm     0.04
$&$     1.63    \pm     0.01    $&$     28      \pm     5       $&$ 
0.09    \pm     0.01    $\\
3C 
41   &       0.794   &       93.8    &$      0.032   \pm     0.005   $&$ 
   0.10    \pm     0.01    $&$     7.28    \pm     0.06    $&$
2.86    \pm     0.02    $&$     17      \pm     4       $&$     0.21 
\pm     0.06    $\\
3C 
41   &       0.794   &       84.8    &$      0.030   \pm     0.004   $&$ 
   0.14    \pm     0.01    $&$     7.49    \pm     0.01    $&$
6.71    \pm     0.01    $&$     40      \pm     7       $&$     0.56 
\pm     0.12    $\\
3C 
44   &       0.660   &       280.0   &$      0.065   \pm     0.008   $&$ 
   0.31    \pm     0.02    $&$     5.90    \pm     0.05    $&$
3.44    \pm     0.02    $&$     28      \pm     4       $&$     0.06 
\pm     0.01    $\\
3C 
44   &       0.660   &       172.2   &$      0.038   \pm     0.004   $&$ 
   0.18    \pm     0.01    $&$     8.35    \pm     0.02    $&$
2.94    \pm     0.01    $&$     28      \pm     4       $&$     0.15 
\pm     0.02    $\\
3C 
54   &       0.827   &       201.9   &$      0.071   \pm     0.008   $&$ 
   0.22    \pm     0.02    $&$     9.74    \pm     0.02    $&$
2.92    \pm     0.01    $&$     70      \pm     15      $&$     0.04 
\pm     0.01    $\\
3C 
54   &       0.827   &       187.6   &$      0.045   \pm     0.006   $&$ 
   0.21    \pm     0.02    $&$     7.86    \pm     0.01    $&$
4.86    \pm     0.01    $&$     48      \pm     7       $&$     0.18 
\pm     0.03    $\\
3C 
114  &       0.815   &       192.1   &$      0.045   \pm     0.003   $&$ 
   0.13    \pm     0.01    $&$     18.09   \pm     0.01
$&$     1.37    \pm     0.002   $&$     72      \pm     15      $&$ 
0.05    \pm     0.01    $\\
3C 
114  &       0.815   &       209.5   &$      0.058   \pm     0.004   $&$ 
   0.16    \pm     0.01    $&$     15.19   \pm     0.01
$&$     1.47    \pm     0.002   $&$     70      \pm     15      $&$ 
0.03    \pm     0.00    $\\
3C 
142.1        &       0.406   &       99.2    &$      0.019   \pm     0.003 
   $&$     0.11    \pm     0.01    $&$     6.77    \pm     0.00
$&$     4.39    \pm     0.005   $&$     13      \pm     2       $&$ 
0.95    \pm     0.17    $\\
3C 
142.1        &       0.406   &       185.1   &$      0.047   \pm     0.008 
   $&$     0.20    \pm     0.03    $&$     9.49    \pm     0.01
$&$     1.82    \pm     0.003   $&$     27      \pm     6       $&$ 
0.06    \pm     0.02    $\\
3C 
169.1        &       0.633   &       131.4   &$      0.039   \pm     0.005 
   $&$     0.09    \pm     0.01    $&$     20.17   \pm     0.01
$&$     0.58    \pm     0.002   $&$     33      \pm     8       $&$ 
0.03    \pm     0.01    $\\
3C 
169.1        &       0.633   &       189.7   &$      0.048   \pm     0.006 
   $&$     0.16    \pm     0.02    $&$     12.98   \pm     0.02
$&$     1.16    \pm     0.003   $&$     34      \pm     7       $&$ 
0.04    \pm     0.01    $\\
3C 
172  &       0.519   &       294.7   &$      0.058   \pm     0.013   $&$ 
   0.24    \pm     0.05    $&$     6.01    \pm     0.11
$&$     2.01    \pm     0.03    $&$     15      \pm     4       $&$ 
0.04    \pm     0.02    $\\
3C 
172  &       0.519   &       333.0   &$      0.119   \pm     0.058   $&$ 
   0.43    \pm     0.21    $&$     14.14   \pm     0.01
$&$     1.92    \pm     0.004   $&$     163     \pm     83      $&$ 
0.01    \pm     0.01    $\\
3C 
441  &       0.707   &       69.4    &$      0.015   \pm     0.001   $&$ 
   0.049   \pm     0.004   $&$     19.16   \pm     0.01
$&$     1.40    \pm     0.002   $&$     28      \pm     6       $&$ 
0.45    \pm     0.06    $\\
3C 
441  &       0.707   &       169.7   &$      0.076   \pm     0.016   $&$ 
   0.33    \pm     0.06    $&$     10.14   \pm     0.02
$&$     3.11    \pm     0.01    $&$     87      \pm     21      $&$ 
0.04    \pm     0.02    $\\
3C 
469.1        &       1.336   &       306.1   &$      0.124   \pm     0.020 
   $&$     0.49    \pm     0.07    $&$     6.97    \pm     0.04
$&$     17.17   \pm     0.07    $&$     368     \pm     79      $&$ 
0.08    \pm     0.02    $\\
3C 
469.1        &       1.336   &       327.5   &$      0.112   \pm     0.012 
   $&$     0.40    \pm     0.04    $&$     13.54   \pm     0.02
$&$     6.48    \pm     0.01    $&$     473     \pm     96      $&$ 
0.04    \pm     0.01    $\\
\hline
\end{tabular}}}
\medskip
All calculations follow WDW and assume $b = 0.25$ except where noted. The top part of the table contains the properties of the previous sample of 20~radio sources recalculated for the currently adopted cosmology.  The bottom part of the table contains the new sample of 11~radio galaxies.
Column~1: source name, Col.~2: redshift, Col.~3: the distance between the core and hotspot,
Col.~4: the source expansion speed, Col.~5: the source expansion speed for $b= 1$,
Col.~6: the half-width of the lobe at a projected distance of 10~kpc along the ridge
line from the hotspot towards the core, Col.~7: the pressure in the lobe at a projected distance of 10~kpc along the ridge line from the hotspot towards the core,
Col.~8: the beam power, Col.~9: the ambient density.
\end{table}