\begin{table}%tA.1
\caption{\label{tabposn}Estimates of velocities at multiple positions in the
lobes in the eleven radio galaxies.}
\par
%\centering
\small
\begin{tabular}{lclrrr}
\hline\hline
Source & Side &    $\theta$ & $\nu_{0T}$ &      $v/c$ ($b=0.25$)  & $v/c$ ($b=1$) \\
         &                               &         arcsec & GHz &        \\
\hline
3C 6.1   &       N       &       5       &$      57      \pm     53 
$&$     0.0629  \pm     0.0303  $&$     0.303   \pm     0.143   $\\
         &               &       7.5     &$      140     \pm     230 
 $&$     0.1510  \pm     0.1219  $&$     0.728   \pm     0.584   $\\
         &               &       10      &$      25      \pm     13 
 $&$     0.0839  \pm     0.0245  $&$     0.404   \pm     0.111   $\\
         &               &       avg     &$ 
 $&$     0.0770  \pm     0.0190  $&$     0.370   \pm     0.090   $\\
3C 6.1   &       S       &       5       &$      14      \pm     4 
$&$     0.0272  \pm     0.0047  $&$     0.107   \pm     0.018   $\\
         &               &       7.5     &$      30      \pm     18 
 $&$     0.0603  \pm     0.0185  $&$     0.236   \pm     0.071   $\\
         &               &       avg     &$ 
 $&$     0.0290  \pm     0.0050  $&$     0.110   \pm     0.020   $\\
3C 34    &       E       &       5       &$      66      \pm     66 
$&$     0.0388  \pm     0.0196  $&$     0.125   \pm     0.063   $\\
         &               &       7.5     &$      32      \pm     18 
 $&$     0.0405  \pm     0.0117  $&$     0.131   \pm     0.038   $\\
         &               &       10      &$      38      \pm     26 
 $&$     0.0591  \pm     0.0200  $&$     0.191   \pm     0.064   $\\
         &               &       12.5    &$      14      \pm     4 
 $&$     0.0450  \pm     0.0071  $&$     0.145   \pm     0.022   $\\
         &               &       15      &$      14      \pm     4 
 $&$     0.0532  \pm     0.0083  $&$     0.172   \pm     0.026   $\\
         &               &       17.5    &$      12      \pm     3 
 $&$     0.0572  \pm     0.0083  $&$     0.185   \pm     0.026   $\\
         &               &       20      &$      7.1     \pm     1.1 
 $&$     0.0507  \pm     0.0051  $&$     0.164   \pm     0.016   $\\
         &               &       avg     &$ 
 $&$     0.0500  \pm     0.0030  $&$     0.160   \pm     0.010   $\\
3C 34    &       W       &       5       &$      18      \pm     7 
$&$     0.0202  \pm     0.0041  $&$     0.063   \pm     0.013   $\\
         &               &       7.5     &$      13      \pm     4 
 $&$     0.0261  \pm     0.0038  $&$     0.081   \pm     0.012   $\\
         &               &       10      &$      19      \pm     69 
 $&$     0.0411  \pm     0.0754  $&$     0.128   \pm     0.234   $\\
         &               &       12.5    &$      7.5     \pm     1.6 
 $&$     0.0324  \pm     0.0037  $&$     0.101   \pm     0.011   $\\
         &               &       15      &$      6.5     \pm     1.0 
 $&$     0.0363  \pm     0.0032  $&$     0.113   \pm     0.009   $\\
         &               &       avg     &$ 
 $&$     0.0298  \pm     0.0020  $&$     0.093   \pm     0.005   $\\
3C 41    &       N       &       2.5     &$      29      \pm     18 
$&$     0.0165  \pm     0.0054  $&$     0.051   \pm     0.017   $\\
         &               &       5       &$      17      \pm     6 
 $&$     0.0256  \pm     0.0051  $&$     0.079   \pm     0.016   $\\
         &               &       7.5     &$      8.6     \pm     2.1 
 $&$     0.0271  \pm     0.0043  $&$     0.084   \pm     0.013   $\\
         &               &       avg     &$ 
 $&$     0.0240  \pm     0.0030  $&$     0.073   \pm     0.008   $\\
3C 41    &       S       &       2.5     &$      33      \pm     22 
$&$     0.0206  \pm     0.0074  $&$     0.094   \pm     0.033   $\\
         &               &       5       &$      5.9     \pm     1.2 
 $&$     0.0175  \pm     0.0028  $&$     0.080   \pm     0.011   $\\
         &               &       avg     &$ 
 $&$     0.0180  \pm     0.0030  $&$     0.080   \pm     0.010   $\\
3C 44    &       N       &       5       &$      18      \pm     8 
$&$     0.0220  \pm     0.0053  $&$     0.104   \pm     0.023   $\\
         &               &       10      &$      17      \pm     7 
 $&$     0.0433  \pm     0.0102  $&$     0.204   \pm     0.045   $\\
         &               &       15      &$      4.2     \pm     0.9 
 $&$     0.0337  \pm     0.0048  $&$     0.159   \pm     0.017   $\\
         &               &       20      &$      16      \pm     8 
 $&$     0.0836  \pm     0.0218  $&$     0.394   \pm     0.096   $\\
         &               &       25      &$      6.5     \pm     1.1 
 $&$     0.0666  \pm     0.0089  $&$     0.314   \pm     0.030   $\\
         &               &       avg     &$ 
 $&$     0.0360  \pm     0.0030  $&$     0.170   \pm     0.010   $\\
3C 44    &       S       &       5       &$      28      \pm     15 
$&$     0.0277  \pm     0.0080  $&$     0.131   \pm     0.036   $\\
         &               &       10      &$      7.6     \pm     1.8 
 $&$     0.0290  \pm     0.0044  $&$     0.137   \pm     0.017   $\\
         &               &       15      &$      5.2     \pm     0.6 
 $&$     0.0358  \pm     0.0041  $&$     0.170   \pm     0.011   $\\
         &               &       20      &$      3.4     \pm     0.3 
 $&$     0.0390  \pm     0.0042  $&$     0.185   \pm     0.010   $\\
         &               &       avg     &$ 
 $&$     0.0340  \pm     0.0030  $&$     0.170   \pm     0.010   $\\
3C 54    &       N       &       2.5     &$      140     \pm     220 
$&$     0.0391  \pm     0.0317  $&$     0.124   \pm     0.100    $\\
         &               &       5       &$      16      \pm     7 
 $&$     0.0267  \pm     0.0058  $&$     0.085   \pm     0.018   $\\
         &               &       7.5     &$      15      \pm     6 
 $&$     0.0394  \pm     0.0084  $&$     0.125   \pm     0.027   $\\
         &               &       10      &$      23      \pm     12 
 $&$     0.0646  \pm     0.0167  $&$     0.205   \pm     0.053   $\\
         &               &       12.5    &$      21      \pm     10 
 $&$     0.0760  \pm     0.0185  $&$     0.241   \pm     0.059   $\\
         &               &       15      &$      15      \pm     5 
 $&$     0.0775  \pm     0.0151  $&$     0.245   \pm     0.047   $\\
         &               &       17.5    &$      15      \pm     6 
 $&$     0.0919  \pm     0.0182  $&$     0.291   \pm     0.057   $\\
         &               &       20      &$      7.4     \pm     1.7 
 $&$     0.0729  \pm     0.0098  $&$     0.231   \pm     0.031   $\\
         &               &       22.5    &$      6.0     \pm     1.2 
 $&$     0.0734  \pm     0.0091  $&$     0.233   \pm     0.028   $\\
         &               &       avg     &$ 
 $&$     0.0510  \pm     0.0030  $&$     0.160   \pm     0.010   $\\
3C 54    &       S       &       2.5     &$      34      \pm     23 
$&$     0.0232  \pm     0.0085  $&$     0.110   \pm     0.039   $\\
         &               &       5       &$      18      \pm     8 
 $&$     0.0344  \pm     0.0086  $&$     0.163   \pm     0.038   $\\
         &               &       7.5     &$      9.8     \pm     2.6 
 $&$     0.0376  \pm     0.0067  $&$     0.178   \pm     0.027   $\\
         &               &       10      &$      7.6     \pm     1.4 
 $&$     0.0442  \pm     0.0066  $&$     0.209   \pm     0.024   $\\
         &               &       12.5    &$      4.9     \pm     0.6 
 $&$     0.0442  \pm     0.0056  $&$     0.209   \pm     0.018   $\\
         &               &       15      &$      4.0     \pm     0.4 
 $&$     0.0480  \pm     0.0060  $&$     0.228   \pm     0.019   $\\
         &               &       avg     &$ 
 $&$     0.0410  \pm     0.0030  $&$     0.200   \pm     0.010   $\\
3C 114   &       N       &       2.5     &$      210     \pm     370 
$&$     0.0463  \pm     0.0406  $&$     0.132   \pm     0.116 $\\
         &               &       5       &$      210     \pm     368 
 $&$     0.0926  \pm     0.0812  $&$     0.264   \pm     0.231   $\\
         &               &       7.5     &$      35      \pm     22 
 $&$     0.0570  \pm     0.0178  $&$     0.162   \pm     0.051   $\\
         &               &       10      &$      7.6     \pm     1.4 
 $&$     0.0353  \pm     0.0039  $&$     0.100   \pm     0.011   $\\
         &               &       12.5    &$      5.4     \pm     0.9 
 $&$     0.0370  \pm     0.0036  $&$     0.105   \pm     0.010   $\\
         &               &       15      &$      2.5     \pm     0.3 
 $&$     0.0304  \pm     0.0027  $&$     0.087   \pm     0.007   $\\
         &               &       17.5    &$      2.7     \pm     0.5 
 $&$     0.0370  \pm     0.0038  $&$     0.105   \pm     0.011   $\\
         &               &       20      &$      3.8     \pm     0.4 
 $&$     0.0498  \pm     0.0037  $&$     0.142   \pm     0.010   $\\
         &               &       avg     &$ 
 $&$     0.0370  \pm     0.0010  $&$     0.100   \pm     0.004   $\\
\hline
3C 114   &       S       &       2.5     &$      86      \pm     110 
$&$     0.0296  \pm     0.0190  $&$     0.083   \pm     0.053 $\\
         &               &       5       &$      24      \pm     12 
 $&$     0.0315  \pm     0.0081  $&$     0.088   \pm     0.023   $\\
         &               &       7.5     &$      14      \pm     6 
 $&$     0.0364  \pm     0.0072  $&$     0.102   \pm     0.020   $\\
         &               &       10      &$      11      \pm     3 
 $&$     0.0423  \pm     0.0061  $&$     0.118   \pm     0.017   $\\
         &               &       12.5    &$      21      \pm     10 
 $&$     0.0740  \pm     0.0179  $&$     0.207   \pm     0.050   $\\
         &               &       15      &$      6.6     \pm     1.5 
 $&$     0.0493  \pm     0.0056  $&$     0.138   \pm     0.016   $\\
         &               &       17.5    &$      6.2     \pm     1.1 
 $&$     0.0557  \pm     0.0050  $&$     0.156   \pm     0.014   $\\
         &               &       20      &$      6.9     \pm     1.3 
 $&$     0.0672  \pm     0.0064  $&$     0.188   \pm     0.018   $\\
         &               &       22.5    &$      4.9     \pm     0.6 
 $&$     0.0634  \pm     0.0040  $&$     0.178   \pm     0.011   $\\
         &               &       avg     &$ 
 $&$     0.0530  \pm     0.0020  $&$     0.150   \pm     0.006   $\\
3C 142.1 
&       N       &       2.5     &$      380     \pm     900     $&$ 
0.0306  \pm     0.0360  $&$     0.185   \pm
0.216   $\\
         &               &       5       &$      140     \pm     190 
 $&$     0.0368  \pm     0.0263  $&$     0.222   \pm     0.156   $\\
         &               &       7.5     &$      96      \pm     96 
 $&$     0.0460  \pm     0.0239  $&$     0.278   \pm     0.139   $\\
         &               &       10      &$      18      \pm     7 
 $&$     0.0267  \pm     0.0062  $&$     0.162   \pm     0.030   $\\
         &               &       12.5    &$      6.5     \pm     1.1 
 $&$     0.0200  \pm     0.0034  $&$     0.121   \pm     0.011   $\\
         &               &       avg     &$ 
 $&$     0.0220  \pm     0.0030  $&$     0.130   \pm     0.010   $\\
3C 142.1 
&       S       &       2.5     &$      14~000   \pm     330~000  $&$ 
0.1279  \pm     1.5354  $&$     0.568   \pm
6.814   $\\
         &               &       5       &$      14~000   \pm     330~000 
 $&$     0.2559  \pm     3.0707  $&$     1.136   \pm     13.628  $\\
         &               &       7.5     &$      61      \pm     57 
 $&$     0.0256  \pm     0.0121  $&$     0.114   \pm     0.053   $\\
         &               &       10      &$      38      \pm     24 
 $&$     0.0269  \pm     0.0088  $&$     0.120   \pm     0.038   $\\
         &               &       12.5    &$      29      \pm     16 
 $&$     0.0291  \pm     0.0083  $&$     0.129   \pm     0.036   $\\
         &               &       15      &$      35      \pm     21 
 $&$     0.0384  \pm     0.0120  $&$     0.170   \pm     0.051   $\\
         &               &       17.5    &$      22      \pm     11 
 $&$     0.0358  \pm     0.0091  $&$     0.159   \pm     0.039   $\\
         &               &       20      &$      38      \pm     24 
 $&$     0.0539  \pm     0.0176  $&$     0.239   \pm     0.076   $\\
         &               &       22.5    &$      18      \pm     8 
 $&$     0.0411  \pm     0.0095  $&$     0.183   \pm     0.040   $\\
         &               &       25      &$      26      \pm     14 
 $&$     0.0556  \pm     0.0153  $&$     0.247   \pm     0.065   $\\
         &               &       27.5    &$      35      \pm     21 
 $&$     0.0704  \pm     0.0220  $&$     0.312   \pm     0.094   $\\
         &               &       30      &$      17      \pm     7 
 $&$     0.0539  \pm     0.0122  $&$     0.239   \pm     0.051   $\\
         &               &       avg     &$ 
 $&$     0.0370  \pm     0.0030  $&$     0.170   \pm     0.010   $\\
3C 169.1 
&       N       &       2.5     &$      540     \pm     1900    $&$ 
0.0460  \pm     0.0827  $&$     0.108   \pm 0.194
$\\
         &               &       5       &$      240     \pm     570 
 $&$     0.0613  \pm     0.0735  $&$     0.144   \pm     0.173   $\\
         &               &       7.5     &$      34      \pm     22 
 $&$     0.0345  \pm     0.0113  $&$     0.081   \pm     0.026   $\\
         &               &       10      &$      26      \pm     15 
 $&$     0.0409  \pm     0.0119  $&$     0.096   \pm     0.028   $\\
         &               &       12.5    &$      4.9     \pm     0.8 
 $&$     0.0219  \pm     0.0020  $&$     0.051   \pm     0.005   $\\
         &               &       avg     &$ 
 $&$     0.0023  \pm     0.0020  $&$     0.053   \pm     0.004   $\\
3C 169.1 
&       S       &       2.5     &$      13~000   \pm     300~000  $&$ 
0.2368  \pm     2.6043  $&$     0.766   \pm
8.424   $\\
         &               &       5       &$      130     \pm     200 
 $&$     0.0474  \pm     0.0380  $&$     0.153   \pm     0.123   $\\
         &               &       7.5     &$      49      \pm     48 
 $&$     0.0431  \pm     0.0210  $&$     0.139   \pm     0.068   $\\
         &               &       10      &$      52      \pm     52 
 $&$     0.0592  \pm     0.0298  $&$     0.191   \pm     0.096   $\\
         &               &       12.5    &$      30      \pm     20 
 $&$     0.0564  \pm     0.0190  $&$     0.182   \pm     0.061   $\\
         &               &       15      &$      14      \pm     6 
 $&$     0.0466  \pm     0.0095  $&$     0.151   \pm     0.030   $\\
         &               &       17.5    &$      15      \pm     6 
 $&$     0.0552  \pm     0.0115  $&$     0.179   \pm     0.037   $\\
         &               &       20      &$      11      \pm     3 
 $&$     0.0541  \pm     0.0083  $&$     0.175   \pm     0.026   $\\
         &               &       22.5    &$      5.0     \pm     0.8 
 $&$     0.0410  \pm     0.0039  $&$     0.133   \pm     0.012   $\\
         &               &       25      &$      4.4     \pm     1.6 
 $&$     0.0431  \pm     0.0082  $&$     0.139   \pm     0.026   $\\
         &               &       avg     &$ 
 $&$     0.0450  \pm     0.0030  $&$     0.140   \pm     0.010   $\\
3C 172   &       N       &       2.5     &$      60      \pm     48 
$&$     0.0121  \pm     0.0050  $&$     0.050   \pm     0.020   $\\
         &               &       5       &$      52      \pm     46 
 $&$     0.0227  \pm     0.0101  $&$     0.093   \pm     0.041   $\\
         &               &       7.5     &$      13      \pm     4 
 $&$     0.0167  \pm     0.0030  $&$     0.069   \pm     0.011   $\\
         &               &       10      &$      130     \pm     240 
 $&$     0.0725  \pm     0.0656  $&$     0.297   \pm     0.268   $\\
         &               &       12.5    &$      18      \pm     7 
 $&$     0.0336  \pm     0.0069  $&$     0.138   \pm     0.026   $\\
         &               &       15      &$      39      \pm     30 
 $&$     0.0588  \pm     0.0228  $&$     0.241   \pm     0.092   $\\
         &               &       17.5    &$      39      \pm     30 
 $&$     0.0686  \pm     0.0266  $&$     0.281   \pm     0.107   $\\
         &               &       20      &$      60      \pm     48 
 $&$     0.0967  \pm     0.0396  $&$     0.396   \pm     0.160   $\\
         &               &       22.5    &$      32      \pm     25 
 $&$     0.0796  \pm     0.0318  $&$     0.326   \pm     0.128   $\\
         &               &       25      &$      79      \pm     86 
 $&$     0.1394  \pm     0.0761  $&$     0.572   \pm     0.309   $\\
         &               &       27.5    &$      32      \pm     22 
 $&$     0.0973  \pm     0.0343  $&$     0.399   \pm     0.138   $\\
         &               &       30      &$      12      \pm     34 
 $&$     0.0659  \pm     0.0107  $&$     0.270   \pm     0.039   $\\
         &               &       32.5    &$      5.4     \pm     1.1 
 $&$     0.0471  \pm     0.0063  $&$     0.193   \pm     0.022   $\\
         &               &       avg     &$ 
 $&$     0.0250  \pm     0.0020  $&$     0.100   \pm     0.008   $\\
3C 172   &       S       &       2.5     &$      440     \pm     1500 
$&$        0.0312  \pm     0.0539  $&$     0.112   \pm     0.193
$\\
         &               &       5       &$      13~000   \pm     270~000 
 $&$     0.3431  \pm     3.4312  $&$     1.227   \pm     12.273  $\\
         &               &       7.5     &$      13~000   \pm     270~000 
 $&$     0.5147  \pm     5.1469  $&$     1.841   \pm     18.410
$\\
\hline
         &               &       10      &$      13~000   \pm     270~000 
 $&$     0.6862  \pm     6.8625  $&$     2.455   \pm     24.547
$\\
         &               &       12.5    &$      110     \pm     180 
 $&$     0.0780  \pm     0.0640  $&$     0.279   \pm     0.229   $\\
         &               &       15      &$      13~000   \pm     270~000 
 $&$     1.0294  \pm     10.2937 $&$     3.682   \pm     36.820
$\\
         &               &       17.5    &$      210     \pm     520 
 $&$     0.1501  \pm     0.1879  $&$     0.537   \pm     0.672   $\\
         &               &       20      &$      13~000   \pm     270~000 
 $&$     1.3725  \pm     13.7250 $&$     4.909   \pm     49.093
$\\
         &               &       22.5    &$      110     \pm     180 
 $&$     0.1404  \pm     0.1152  $&$     0.502   \pm     0.412   $\\
         &               &       25      &$      210     \pm     520 
 $&$     0.2145  \pm     0.2685  $&$     0.767   \pm     0.960   $\\
         &               &       27.5    &$      15      \pm     5 
 $&$     0.0629  \pm     0.0113  $&$     0.225   \pm     0.040   $\\
         &               &       32.5    &$      13      \pm     9 
 $&$     0.0708  \pm     0.0230  $&$     0.253   \pm     0.082   $\\
         &               &       avg     &$ 
 $&$     0.0650  \pm     0.0100  $&$     0.230   \pm     0.030   $\\
3C 441   &       N       &       2.5     &$      26      \pm     18 
$&$     0.0128  \pm     0.0043  $&$     0.041   \pm     0.014   $\\
         &               &       5       &$      11      \pm     3 
 $&$     0.0165  \pm     0.0024  $&$     0.052   \pm     0.007   $\\
         &               &       avg     &$ 
 $&$     0.0156  \pm     0.0020  $&$     0.050   \pm     0.007   $\\
3C 441   &       S       &       2.5     &$      1500 \pm        9900 
$&$        0.1076  \pm     0.3589  $&$     0.464   \pm
1.546   $\\
         &               &       5       &$      86      \pm     100 
 $&$     0.0517  \pm     0.0314  $&$     0.223   \pm     0.134   $\\
         &               &       7.5     &$      150     \pm     190 
 $&$     0.1020  \pm     0.0652  $&$     0.439   \pm     0.279   $\\
         &               &       10      &$      34      \pm     23 
 $&$     0.0646  \pm     0.0235  $&$     0.278   \pm     0.099   $\\
         &               &       12.5    &$      150     \pm     190 
 $&$     0.1699  \pm     0.1086  $&$     0.732   \pm     0.465   $\\
         &               &       15      &$      34      \pm     24 
 $&$     0.0969  \pm     0.0352  $&$     0.417   \pm     0.148   $\\
         &               &       17.5    &$      10      \pm     3 
 $&$     0.0628  \pm     0.0100  $&$     0.271   \pm     0.038   $\\
         &               &       20      &$      16      \pm     5 
 $&$     0.0891  \pm     0.0177  $&$     0.384   \pm     0.070   $\\
         &               &       avg     &$ 
 $&$     0.0699  \pm     0.0080  $&$     0.300   \pm     0.030   $\\
3C 469.1 
&       N       &       2.5     &$      150     \pm     160     $&$ 
0.1145  \pm     0.0617  $&$     0.456   \pm
0.245   $\\
         &               &       5       &$      840     \pm     3800 
 $&$     0.5444  \pm     1.2266  $&$     2.173   \pm     4.896   $\\
         &               &       7.5     &$      9.1     \pm     1.9 
 $&$     0.0848  \pm     0.0132  $&$     0.339   \pm     0.051   $\\
         &               &       10      &$      18      \pm     6 
 $&$     0.1584  \pm     0.0341  $&$     0.632   \pm     0.134   $\\
         &               &       avg     &$ 
 $&$     0.0950  \pm     0.0120  $&$     0.380   \pm     0.050   $\\
3C 469.1 
&       S       &       2.5     &$      130     \pm     200     $&$ 
0.1050  \pm     0.0793  $&$     0.383   \pm
0.288   $\\
         &               &       5       &$      130     \pm     210 
 $&$     0.2100  \pm     0.1689  $&$     0.766   \pm     0.615   $\\
         &               &       7.5     &$      13      \pm     2 
 $&$     0.0985  \pm     0.0123  $&$     0.359   \pm     0.042   $\\
         &               &       10      &$      9.3     \pm     2.0 
 $&$     0.1106  \pm     0.0148  $&$     0.403   \pm     0.051   $\\
         &               &       12.5    &$      9.3     \pm     2.0 
 $&$     0.1382  \pm     0.0185  $&$     0.504   \pm     0.063   $\\
         &               &       15      &$      11      \pm     3 
 $&$     0.1800  \pm     0.0297  $&$     0.656   \pm     0.104   $\\
         &               &       17.5    &$      8.4     \pm     1.7 
 $&$     0.1838  \pm     0.0239  $&$     0.670   \pm     0.081   $\\
          &              &       avg      & 
 &$
0.1200   \pm    0.0080  $&$     0.450   \pm     0.030   $\\
\hline
\end{tabular}
\medskip
Column~1: source name. Column~2: side of the source on which the spectral aging was determined. Column~3: the distance from the hotspot. The estimated error is 0.5~arcsec.
Column~4: the estimated break frequency.
Column~5: the estimated hot spot advance speed assuming the magnetic field is equal to 0.25 the averaged equipartition value given in Table~\ref{tabaging}.
Column6: the estimated hot spot advance speed assuming the magnetic field is equal to
the averaged equipartition value given in Table~\ref{tabaging}. The last row for each side gives the weighted mean velocity.
\end{table}