\begin{table}%t4
\caption{\label{tab:cr_tp_flux density}Integrated total power flux densities. $S_{\rm i}$~is the total integrated flux density and $S_{\rm e}$~is the flux density of the extended emission only. The error of the flux densities was calculated as the quadratic sum of a~5\% calibration error and the baselevel error.}
%\centering
\small
\begin{tabular}{lllll}
\hline\hline 
$\lambda~{\rm [cm]}$ \T\B& Instrument & $S_{\rm i}~{\rm [Jy]}$ & $S_{\rm e}~{\rm [Jy]}$\\
\hline
90 \T & VLA & $16.5\pm 1.9$ & $12.5\pm 1.9$\\ 
20 & VLA & $6.3\pm 1.1$ & $4.2\pm 1.1$\\ 
6.2 & VLA + Effelsberg & $2.71\pm 0.14$ & $1.44\pm 0.07$\\ 
3.6 \B & Effelsberg & $1.66\pm 0.08$ & $0.68\pm0.04$\\
\hline
\end{tabular}
\end{table}