\begin{table}%t2
 \caption{\label{LWS_obs} ISO-LWS [O~I] line fluxes and line ratios for the VLA~1623 outflow and the neighbouring \ro\ PDR.}
 %\centerline
{
\par
\begin{tabular}{lllllllll}
\hline 
\hline \noalign{\smallskip}
TDT        & RA(J2000)      & Dec(J2000)                & \powten{12}  $F_{63~\mu {\rm m} }$    &  $S/N_{63}$  & \powten{12}  $F_{145~\mu {\rm m} }$  & $S/N_{145}$  & Project Name/ & Comment   \\    number  & (h   m   s)         & (\adeg\     \amin\     \asec) &  (\ecs)                                                 &                         &  (\ecs)                                                        &                          &  Position           &                       \\     
\noalign{\smallskip}
\hline
  \noalign{\smallskip}
{\bf Flow}       &                             &                        &                                  &                       &                                  &           &                                      &                       \\
29200533$^a$ & 16 26 26.27      &  $-24$ 24 30 & $18.52 \pm 1.29$ &     14             &  $4.47  \pm 1.50$  &   2.6  &    VLA 1623                & Origin (flow 0\asec\ offset)   \\			  
29200534$^b$ & 16 26 17.22      & $-24$ 23 06  & $22.54 \pm 0.80$ &     28             &  $4.22  \pm 0.86$  &   4.9  &    VLA 1623 flow(1, 1) &  150\asec\ NW  (PA=304\adeg)\\
29200534          & 16 26 23.25      & $-24$ 24 02  & $18.52 \pm 1.27$ &     15             &  $4.47  \pm 1.35$  &   3.3  &    VLA 1623 flow(2, 1) &  \phantom{1}50\asec\ NW (PA=304\adeg)\\
29200534          & 16 26 29.29      & $-24$ 24 58  & $21.92 \pm 1.00$ &     22             &  $8.94  \pm 1.62$  &   5.5  &    VLA 1623 flow(3, 1) & \phantom{1}50\asec\ SE   (PA=124\adeg) \\
\noalign{\smallskip}
\hline
  \noalign{\smallskip}  
{\bf PDR}   &                             &                        &                                  &         &                                   &        &                                     &       \\
45400801 & 16 25 55.56      & $-24$ 25 39 & $10.08  \pm 0.77$ &   13  &  $4.02  \pm 0.80$   & 5.0 & ROPH\_EW ew2      &  \about south 1\amin\ west 7\amin \\
45400801 & 16 26 08.74      & $-24$ 25 40 & $12.66  \pm 0.62$ &    20 &  $4.92  \pm 1.09$   & 4.5 &  ROPH\_EW ew3     &  \about south 1\amin\ west 4\amin \\          
45400801 & 16 26 21.92      & $-24$ 25 40 & $10.56  \pm 0.81$ &   13  &  $3.45  \pm  0.60$  & 5.8 & ROPH\_EW ew4      &  \about south 1\amin\ west 1\amin \\          
45400801 & 16 26 35.10      & $-24$ 25 41 & $12.66  \pm 0.36$ &    35 &  $4.41  \pm 0.86$   &  5.1 &  ROPH\_EW ew5    &  \about south 1\amin\ east 2\amin \\
{\bf PDR$_{\rm ave}$}$^c$       &      &                         & $11.49  \pm 0.64$ &   18 &  $4.20 \pm  0.86$   & 4.9 &                                     &    \\   
   \noalign{\smallskip}      
  \hline
 \noalign{\smallskip}   
{\bf Offset}$^d$ &16 26 35.32 & $-24$ 25 54  & $\phantom{1}9.88 \pm 1.13$ & \phantom{1}9 & $3.96 \pm 0.93$   &   4.2  &    VLA 1623 flow(4,1) & 150\asec\ SE (PA=124\adeg) \\
\noalign{\smallskip} 
\hline
  \noalign{\smallskip}            
 \noalign{\smallskip} 
{\bf Flow$-$PDR$_{\rm ave}$}&  &                &   11.05                    &          &   0.02                        &          &   552 = Line Ratio     &   150\asec\ NW (PA=304\adeg)    \\
                    &                            &                         &  \phantom{1}7.03 &          &   0.27                        &          &   \phantom{1}26        &   \phantom{1}50\asec\ NW  (PA=304\adeg)  \\  
                    &                            &                         &  \phantom{1}7.96 &          &   0.27                        &          &   \phantom{1}29        &  Origin (flow 0\asec\ offset)    \\      
{\bf Flow$-$Offset} &              &                         & 12.66                      &          &  0.26                        &           &    \phantom{1}50 =  Line Ratio       &  150\asec\ NW (PA=304\adeg)\\
                             &                   &                         &  \phantom{1}8.64 &          &  0.48                        &           &   \phantom{1}18        &  \phantom{1}50\asec\ NW (PA=304\adeg)\\   
                             &                   &                         &  \phantom{1}8.64 &          &  0.51                        &           &   \phantom{1}17        & Origin (flow 0\asec\ offset)   \\	
 \noalign{\smallskip}
  \hline
\noalign{\smallskip}
{\bf $\langle$Flow -- PDR$_{\rm ave}$$\rangle$}  &   &  &  \phantom{1}8.68  &            &  0.27                        &           &  $>$25                         &        \\              
{\bf $\langle$Flow -- Offset$\rangle$}  &    &                  &   \phantom{1}9.98 &            & 0.41                         &          &   \phantom{1}24          &                \\
 \noalign{\smallskip}
  \hline
%  \noalign{\smallskip}
  \end{tabular}}
  \medskip
  Notes to the Table:  $^a$  Centre position related to the strip map (TDT 29200534); 
 $^b$ which is  along position angle 124\adeg\ ($\pm 180$\adeg) with 150\asec\ spacings of 4 individual pointings;
  $^c$ the surrounding PDR provides one type of background estimate;
  $^d$ TDT 29200534: this position of the strip scan is outside the flow, yet close enough to serve as another reference position for background estimation. 
\end{table}