\begin{table}%t2
%\centering
\par
\caption{\label{tab:ccdloc}In-flight position and orientation of the AS and PF detectors in the focal plane reference system, as derived during the commissioning run.}
\begin{tabular}{l l c}
\par
		\hline\hline
			CCD & Parameter & Value  \\
			\hline
			A1  & $X(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $-14$ microns   \\
			%\hline
			  &  $Y(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $ -20$ microns   \\
			%\hline
			 & Rotation angle in the focal plane reference system & $ -0.03$  degrees  \\
			\hline
			A2  & $X(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $-9$ microns   \\
			%\hline
			  &  $Y(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $ -2$ microns   \\
			%\hline
			 & Rotation angle in the focal plane reference system & $ -0.05$  degrees  \\
			\hline
			E1  & $X(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $-60$ microns   \\
			%\hline
			  &  $Y(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $ -11$ microns   \\
			%\hline
			 & Rotation angle in the focal plane reference system & $ -0.01$  degrees  \\
			\hline
			E2  & $X(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $-43$ microns   \\
			%\hline
			  &  $Y(1,1)$ -- coordinate offset of the first pixel in the focal plane reference system & $ +60$ microns   \\
			%\hline
			 & Rotation angle in the focal plane reference system & $ -0.01$  degrees  \\
\hline
		\end{tabular}
\end{table}