\begin{table}%t2
      \caption{\label{tab3_hrdata}Summary of the AMBER observations of \object{IRC+10420} and the calibrator star HD~232078 in high-spectral resolution mode from Oct 14, 2008 using the UT telescope configuration UT1-UT2-UT4.}
     %\centerline
{\begin{tabular}{lccccc}
            \hline
            \noalign{\smallskip}
            ${\rm object}$& ${\rm UTC}$& $N_{\rm frames}$& $B_{\rm p}$   & PA      & ${\rm seeing}$\\
                      &            &               & [{\rm m}]   & $[\degr]$ & $[\arcsec]$   \\
             \noalign{\smallskip}
            \hline
            \noalign{\smallskip}
	    ${\rm \irc}$      & 00:26:40  & 125            & 54--129      & 36--75   & 0.9\\
	    ${\rm HD~232078}$ & 00:03:59  & 125            & 51--130      & 37--78   & 1.1\\
            \hline
         \end{tabular}}
         \medskip
\par
All measurements were carried out using the fringe tracker FINITO and with an exposure time of 3~s. 
       The uniform-disk diameter of HD~232078 (spectral type K3IIp), $d_{\rm UD} = 0.74\pm0.1$~mas,
       was taken from the CHARM2 catalogue \citep{charm2}. $N_{\rm frames}$ is the total number of recorded frames.
       For the meaning of the other columns, see Table~\ref{tab1_lrdata}.
   \end{table}