\begin{table}%t1
\caption{\label{tab:ratio_errors}The flux ratio (Ba/Bb) of \epsba, Bb~in the observed FORS2 and ISAAC~filters and the effective wavelength and half-power width of those filters.}
\small%\centerline
 {
\begin{tabular}{clll}
  \hline
  \hline\noalign{\smallskip}
  Observed passband &  Ratio (Ba/Bb)  & $\lambda_{\rm{eff}}~(\mu$m)  &  $\Delta\lambda~(\mu$m)  \\
  \hline
  $V$ & 9.82 $\pm$ 0.66             & 0.554 & 0.112 \\ 
  $R$ & 4.81 $\pm$ 0.07             & 0.655 & 0.165 \\
  $I$ & 5.04 $\pm$ 0.05             & 0.768 & 0.138 \\
  $z$ & 3.85 $\pm$ 0.03             & 0.910 & 0.131 \\
  $J$ & 2.28 $\pm$ 0.02             & 1.25  & 0.29  \\
  $H$ & 5.27 $\pm$ 0.06             & 1.65  & 0.30  \\
  $K_{\rm{S}}$ & 7.12 $\pm$ 0.02     & 2.16  & 0.27  \\
  $L$ & 4.50 $\pm$ 0.16             & 3.78  & 0.58  \\
  $M_{\rm{NB}}$ & 1.35 $\pm$ 0.15    & 4.66 & 0.10 \\
  \hline
\end{tabular}}
\medskip
See Appendix~\ref{sec:phot_calib} for a description of photometric calibration and transformation to standard systems. All except the $V$-band ratio were measured using PSF-fitting (see~Sect.~\ref{sec:opt_phot}).
\end{table}