\begin{table}%t5
\caption{\label{tab:fullres}Full resolution $K$-band imaging. Source parameters.}
\small%\centerline
 {
\begin{tabular}{lllr}
\hline                                     
\hline\noalign{\smallskip}
\multicolumn{1}{c}{Source name} & \multicolumn{1}{c}{RA} & 
\multicolumn{1}{c}{Dec} & \multicolumn{1}{c}{$S_{\rm int}\pm 1\sigma$} \\
     & \multicolumn{1}{c}{(J2000)} & \multicolumn{1}{c}{(J2000)}   
&  \multicolumn{1}{c}{(mJy)} \\
\hline
J224547-400324 &  22 45 47.67 & --40 03 23.4  &     $25.70   \pm 0.22$   \\
J224822-401808$(^a)$ &  22 48 21.99 & --40 18 07.8  &  $3.22    \pm 0.24$  \\
J225004-402412$(^b)$ &    &  &    $1.70     \pm 0.20$   \\
J225034-401936$(^b)$ &    &  &    $7.15    \pm 0.31$   \\
J225057-401522 &  22 50 57.73  & --40 15 22.3 &    $2.21    \pm 0.24$   \\
J225249-401256$(^b)$ &    &  &    $0.63     \pm 0.13$   \\
J225344-401928 &  22 53 44.89  & --40 19 27.2 &    $2.17     \pm 0.08$   \\
\hline
\end{tabular}}
\medskip
$(^a)$ Low surface brightness flux present to the right of the source. Including it we get $S=4.3$~mJy. \\ 
$(^b)$ Coordinates are given only for Gaussian fitted sources. Fluxes for multi-component and/or low $S/N$~sources were obtained by summing the pixels over the entire source. 
\vspace{2mm}\end{table}