\begin{table}%t1
\caption{\label{t:modelparam}Basic parameters of the RHD models (mostly 2D and only one~3D).}
%\centering
\par
\begin{tabular}{lrrrrrrrrr}
\hline\hline \noalign{\smallskip}
Model & p & $n_x \times n_z$ & $x \times z$ & $t_0 - t_1$ & $C_{\rm Cour}$ & $s_{\rm in}$ & $T_{\rm eff,sta}$ & $T_{\rm eff}$ & $T_{\rm opa}$ \\
  &   &   & km $\times$ km & 10$^3$ s &   & erg~K$^{-1}$~g$^{-1}$ & K & K & K \\
\hline\noalign{\smallskip}
mt09g50mm00n10   & d & 400 $\times$ 430 & 220 $\times$  94 &     90--130 & 0.30 & 0.671 $\times$ $10^9$ &  900 &  897 & 1000 \\
mt09g50mm00n11   & d & 400 $\times$ 410 & 220 $\times$  90 &    240--275 & 0.30 & 0.671 $\times$ $10^9$ &  900 &  897 & 1000 \\
mt10g50mm00n03   & d & 400 $\times$ 400 & 240 $\times$  96 &    140--195 & 0.27 & 0.683 $\times$ $10^9$ & 1000 & 1030 & 1000 \\
mt11g50mm00n05   & d & 400 $\times$ 356 & 260 $\times$  92 &    245--285 & 0.30 & 0.690 $\times$ $10^9$ & 1100 & 1114 & 1800 \\
mt12g50mm00n01   & s & 400 $\times$ 336 & 280 $\times$  94 &    110--190 & 0.40 & 0.701 $\times$ $10^9$ & 1200 & 1226 & 1800 \\
mt12g50mm00n07   & s & 400 $\times$ 380 & 280 $\times$ 106 &     80--150 & 0.40 & 0.701 $\times$ $10^9$ & 1200 & 1228 & 1800 \\
mt12g50mm00n10   & s & 400 $\times$ 336 & 280 $\times$  94 &    270--370 & 0.37 & 0.701 $\times$ $10^9$ & 1200 & 1224 & 1800 \\
mt13g50mm00n01   & s & 400 $\times$ 270 & 300 $\times$ 100 &     80--190 & 0.40 & 0.711 $\times$ $10^9$ & 1300 & 1335 & 1800 \\
mt13g50mm00n02   & d & 400 $\times$ 270 & 300 $\times$ 100 &    130--200 & 0.40 & 0.711 $\times$ $10^9$ & 1300 & 1336 & 1800 \\
mt13g50mm00n03   & s & 400 $\times$ 270 & 300 $\times$ 100 &    250--390 & 0.35 & 0.711 $\times$ $10^9$ & 1300 & 1333 & 1800 \\
mt14g50mm00n01   & s & 400 $\times$ 270 & 320 $\times$ 106 &     40--140 & 0.40 & 0.719 $\times$ $10^9$ & 1400 & 1436 & 1800 \\
mt14g50mm00n02   & s & 400 $\times$ 270 & 320 $\times$ 106 &    140--280 & 0.40 & 0.719 $\times$ $10^9$ & 1400 & 1437 & 1800 \\
mt15g50mm00n01   & s & 400 $\times$ 270 & 340 $\times$ 113 &     50--140 & 0.40 & 0.728 $\times$ $10^9$ & 1500 & 1533 & 1800 \\
mt15g50mm00n02   & s & 400 $\times$ 270 & 340 $\times$ 113 &    150--190 & 0.40 & 0.728 $\times$ $10^9$ & 1500 & 1533 & 1800 \\
mt15g50mm00n03   & s & 400 $\times$ 270 & 340 $\times$ 113 &    260--380 & 0.30 & 0.728 $\times$ $10^9$ & 1500 & 1533 & 1800 \\
mt15g50mm00n04   & s & 300 $\times$ 270 & 340 $\times$ 113 &     40--150 & 0.30 & 0.728 $\times$ $10^9$ & 1500 & 1532 & 1800 \\
mt15g50mm00n06   & s & 300$^2$ $\times$ 270 & 340$^2$ $\times$ 113 &     10--15 & 0.30 & 0.728 $\times$ $10^9$ & 1500 & 1532 & 1800 \\
mt15g50mm00n07   & s & 400 $\times$ 300 & 340 $\times$ 127 &     70--150 & 0.30 & 0.728 $\times$ $10^9$ & 1500 & 1533 & 1800 \\
mt16g50mm00n06   & s & 400 $\times$ 366 & 352 $\times$ 128 &     20--190 & 0.40 & 0.737 $\times$ $10^9$ & 1600 & 1648 & 1800 \\
mt17g50mm00n02   & s & 400 $\times$ 352 & 380 $\times$ 133 &     40--190 & 0.40 & 0.747 $\times$ $10^9$ & 1700 & 1757 & 1800 \\
mt18g50mm00n07   & s & 400 $\times$ 343 & 400 $\times$ 137 &     40--190 & 0.40 & 0.756 $\times$ $10^9$ & 1800 & 1858 & 1800 \\
mt19g50mm00n02   & s & 400 $\times$ 334 & 420 $\times$ 140 &     40--80 & 0.40 & 0.765 $\times$ $10^9$ & 1900 & 1953 & 1800 \\
mt19g50mm00n03   & s & 400 $\times$ 334 & 420 $\times$ 140 &    120--290 & 0.30 & 0.765 $\times$ $10^9$ & 1900 & 1953 & 1800 \\
mt20g50mm00n05   & s & 400 $\times$ 362 & 380 $\times$ 137 &     40--210 & 0.20 & 0.775 $\times$ $10^9$ & 2000 & 2052 & 1800 \\
mt22g50mm00n05   & s & 400 $\times$ 351 & 400 $\times$ 140 &     70--150 & 0.20 & 0.798 $\times$ $10^9$ & 2200 & 2247 & 1800 \\
mt24g50mm00n01   & s & 400 $\times$ 344 & 420 $\times$ 144 &     70--190 & 0.20 & 0.825 $\times$ $10^9$ & 2400 & 2426 & 1800 \\
mt26g50mm00n01   & s & 400 $\times$ 353 & 420 $\times$ 148 &     70--140 & 0.20 & 0.859 $\times$ $10^9$ & 2600 & 2597 & 1800 \\
mt26g50mm00n02   & s & 400 $\times$ 353 & 420 $\times$ 148 &     70--140 & 0.20 & 0.859 $\times$ $10^9$ & 2600 & 2611 & 2800 \\
mt28g50mm00n01   & s & 400 $\times$ 357 & 440 $\times$ 157 &     70--140 & 0.20 & 0.905 $\times$ $10^9$ & 2800 & 2801 & 2800 \\
mt28g50mm00n02   & s & 400 $\times$ 380 & 440 $\times$ 167 &     40--100 & 0.20 & 0.905 $\times$ $10^9$ & 2800 & 2801 & 2800 \\
\hline
\end{tabular}
\tablefoot {The columns show model name, numerical precision (single or double), horizontal~$\times$ vertical resolution, horizontal~$\times$ vertical size [km~$\times$~km], time span used for averaging [10$^3$~s], Courant number, entropy of the material in the deeper layers [erg~K$^{-1}$~g$^{-1}$], effective temperature of the PHOENIX~model used for the start file~[K], effective temperature of the RHD~model versus the average time span~[K], and effective temperature of the reference atmosphere used for the opacity table~[K].}
\vspace*{5mm}
\end{table}