\begin{table}%t3
\caption{\label{tab:sed_fitting_results} Results of the SED fitting, with the parameters defined in the~text.}
%\centering
\par
\begin{tabular}{lllllllllllll}
\hline\hline \noalign{\smallskip}
Name & $z_{\rm phot}$ & $\delta z_{\rm phot,min}$ & $\delta z_{\rm phot,max}$ & $\chi^2_\nu$ & $N_{\rm D.O.F.}$ & Dust   & Age & $\Theta$ & $\theta_{\rm view}$ & $f_{\rm AGN}$ & Notes\\[2pt]
\hline
    LOCK850.001 &  5.30 &  1.10 &  0.46 &   0.98 &   8 & SMC &   50 &    1.6 &    35  & 0.73 & \\
    LOCK850.002 &  3.68 &  0.34 &  0.24 &   4.15 &   8 & LMC &   50 &    1.2 &     5  & 0.77 & I\\ 
    LOCK850.003 &  3.80 &  0.22 &  0.20 &   6.67 &   8 & SMC &   50 &    2.0 &     0  & 0.70 & \\ 
   LOCK850.003B &  6.56 &  1.14 &  0.44 &   7.15 &   8 &  MW &  600 &    2.2 &    35  & 0.98 & D, C \\ 
    LOCK850.004 &  3.76 &  0.56 &  2.90 &   2.77 &   9 & SMC &   50 &    1.6 &    45  & 0.08 & U \\ 
   LOCK850.004B &  6.54 &  1.88 &  0.46 &   3.54 &   7 & SMC &  400 &    1.8 &    45  & 0.42 & U \\      LOCK850.005 &  6.14 &  0.60 &  0.44 &   10.02&   6 & SMC &   10 &    1.2 &    30  & 0.86 & C \\
    LOCK850.006 &  5.58 &  1.94 &  1.41 &   3.31 &   8 & SMC &   70 &    2.0 &    42.5& 0.20 & I \\
    LOCK850.007 &  2.56 &  0.60 &  4.44 &   0    &  --3 & SMC &   50 &    0.3 &    10  & 0.18 & I \\
    LOCK850.008 &  0.22 &  0.06 &  6.78 &   0    &  --4 & SMC &  200 &    0.3 &     0  & 0.00 & I \\
    LOCK850.009 &  2.30 &  0.54 &  0.70 &   2.36 &   6 & SMC &  400 &    1.4 &    32.5& 0.56 & U, X \\
   LOCK850.009B &  1.18 &  0.46 &  0.42 &   2.10 &   8 &  MW &  600 &    1.8 &     0  & 0.00 & U\\
   LOCK850.010B &  3.28 &  0.68 &  0.52 &   3.05 &   5 & SMC &   50 &    1.2 &    90 & 0.00\\
    LOCK850.011 &  1.24 &  0.32 &  0.40 &   2.38 &   6 &  MW &  500 &    1.4 &    15 & 0.55 & X \\
    LOCK850.012 &  2.26 &  0.36 &  1.45 &   2.03 &   7 & SMC &  200 &    1.6 &     0 & 0.37 & I \\
    LOCK850.013 &  0.50 &  0.26 &  0.20 &   2.36 &   7 & SMC &  600 &    2.0 &    7.5& 0.09 & X \\
    LOCK850.014 &  3.06 &  0.44 &  0.36 &   3.72 &   7 & SMC &   50 &    1.8 &    50 & 0.01\\
    LOCK850.015 &  1.40 &  0.84 &  0.40 &   3.79 &   8 & SMC &  400 &    0.3 &    27.5& 0.11\\
   LOCK850.015B &  1.36 &  0.18 &  0.16 &   2.54 &   8 & SMC &  500 &    0.4 &    7.5& 0.32 & D\\ 
\hline
    LOCK850.016 &  6.58 &  0.54 &  0.42 &   5.22 &   7 & SMC &   10 &    1.2 &    40 & 0.44\\
    LOCK850.017 &  3.48 &  1.18 &  0.34 &   2.19 &   5 & SMC &  100 &    2.6 &    7.5& 0.50 & U\\
   LOCK850.017B &  4.20 &  0.68 &  1.98 &   1.72 &   5 & LMC &   50 &    1.4 &     0 & 0.65 & U\\
    LOCK850.019 &  3.94 &  0.24 &  1.92 &   1.11 &   5 & SMC &   50 &    2.0 &     5 & 0.69 & I \\
    LOCK850.021 &  0.86 &  0.36 &  6.14 &   0.91 &   6 & SMC &  500 &    0.4 &    17.5 & 0.15 & I \\     LOCK850.022 &  3.10 &  0.90 &  0.40 &   2.24 &   6 &  MW &  600 &    5.0 &     0 & 0.96 \\
    LOCK850.024 &  2.72 &  0.70 &  0.56 &   2.26 &   5 & SMC &   30 &    1.8 &     0 & 0.24\\
    LOCK850.026 &  3.48 &  1.24 &  0.46 &   3.23 &   6 & SMC &   30 &    1.6 &     0 & 0.74 & I\\
    LOCK850.027 &  1.34 &  0.18 &  0.34 &   2.97 &   6 &  MW &  600 &    2.2 &     0 & 0.66\\
    LOCK850.028 &  3.66 &  0.58 &  0.20 &   1.63 &   6 & SMC &   50 &    2.2 &    7.5& 0.50\\
    LOCK850.029 &  4.44 &  3.38 &  2.56 &   0.23 &   5 & SMC &  100 &    1.8 &     0 & 0.96 & I \\
    LOCK850.030 &  2.70 &  1.04 &  0.53 &   2.03 &   6 & SMC &   50 &    0.9 &    50 & 0.00\\
    LOCK850.031 &  1.12 &  0.50 &  1.40 &   2.08 &   5 & SMC &  400 &    0.7 &   17.5& 0.46 & X \\
    LOCK850.033 &  2.78 &  0.66 &  0.70 &   4.75 &   6 & LMC &   70 &    1.2 &    50 & 0.00\\
    LOCK850.034 &  4.14 &  0.45 &  2.02 &   3.19 &   6 & LMC &   50 &    1.2 &    90 & 0.00\\
    LOCK850.035 &  5.24 &  3.26 &  1.76 &   0.72 &   5 & SMC &   70 &    2.0 &    7.5& 0.94 & I\\
   LOCK850.035B &  2.20 &  0.28 &  0.78 &   4.53 &   5 &  MW &  600 &    2.2 &     0 & 0.66 & D\\
    LOCK850.036 &  0.92 &  0.54 &  6.08 &   0    &  --4 & SMC &  200 &    0.3 &     0 & 0.00 & I\\
   LOCK850.037B &  1.26 &  0.46 &  1.00 &   1.84 &   5 & SMC &  300 &    1.4 &   22.5& 0.38 & X \\
    LOCK850.038 &  1.36 &  0.30 &  0.30 &   1.11 &   6 &  MW &  300 &    2.4 &    20 & 0.30\\
    LOCK850.039 &  0.92 &  0.74 &  6.08 &   0    &  --4 & SMC &  200 &    0.3 &     0 & 0.00 & I\\
    LOCK850.040 &  2.24 &  1.64 &  0.34 &   2.02 &   5 &  MW &  400 &    1.8 &     0 & 0.10 & X \\
   LOCK850.041B &  2.44 &  0.94 &  1.38 &   3.38 &   6 & LMC &   50 &    2.2 &    40 & 0.31 \\ 
    LOCK850.041 &  1.60 &  0.44 &  0.10 &   1.61 &   7 & LMC &  200 &    2.4 &    7.5& 0.31\\
    LOCK850.043 &  1.38 &  0.70 &  0.66 &   2.03 &   7 & SMC &  200 &    1.6 &   27.5& 0.42 & U,X \\
   LOCK850.043B &  1.60 &  0.58 &  0.40 &   2.21 &   7 & SMC &  100 &    2.0 &     0 & 0.22 & U,X \\     LOCK850.047 &  3.82 &  0.20 &  0.40 &   1.26 &   7 & LMC &   30 &    3.0 &   37.5& 0.40\\
    LOCK850.048 &  4.18 &  0.86 &  2.16 &   1.70 &   6 & SMC &   10 &    1.6 &    90 & 0.15 \\
    LOCK850.052 &  1.42 &  0.32 &  0.76 &   3.77 &   6 & SMC &  600 &    1.0 &     0 & 0.73 & U\\
   LOCK850.052B &  3.64 &  0.68 &  0.58 &   5.73 &   5 & SMC &  600 &    1.4 &     5 & 0.97 & U\\
    LOCK850.053 &  2.22 &  0.40 &  0.64 &   2.25 &   5 &  MW &  600 &    2.4 &     0 & 0.64 & X\\
    LOCK850.060 &  2.46 &  0.90 &  2.90 &   2.27 &   6 &  MW &  600 &    1.2 &     0 & 0.64 \\
    LOCK850.063 &  4.98 &  0.88 &  0.88 &   0.42 &   7 &  MW &  600 &    2.6 &   32.5& 0.96 & I\\
    LOCK850.064 &  2.10 &  1.41 &  1.28 &   0.98 &   6 & LMC &   50 &    2.2 &     0 & 0.27 & I \\     LOCK850.066 &  3.72 &  0.00 &  1.30 &   0.61 &   5 & SMC &   30 &    0.7 &    50 & 0.03\\
    LOCK850.067 &  7.00 &  0.72 &  0.00 &   3.33 &   6 &  MW &  400 &    3.0 &    40 & 0.83\\
    LOCK850.070 &  0.62 &  0.22 &  0.36 &   0.61 &   6 &  MW &  500 &    1.8 &   22.5& 0.05 & X \\
    LOCK850.071 &  2.24 &  1.48 &  0.88 &   1.91 &   6 &  MW &  600 &    1.8 &     0 & 0.67 & X \\
    LOCK850.073 &  1.72 &  0.96 &  1.88 &   0.64 &   6 & LMC &  100 &    2.0 &    50 & 0.00\\
   LOCK850.073B &  2.26 &  1.52 &  1.30 &   1.17 &   4 &  MW &  400 &    2.4 &   37.5& 0.45 & D \\
    LOCK850.075 &  1.28 &  0.00 &  2.54 &   1.30 &   3 &  MW &  400 &    2.2 &    45 & 0.42 \\
    LOCK850.076 &  0.48 &  0.14 &  0.12 &   2.22 &   8 & SMC &  600 &    1.0 &    7.5& 0.06 & X?\\
    LOCK850.077 &  3.20 &  2.62 &  0.48 &   2.77 &   7 & SMC &   50 &    1.2 &    40 & 0.00 & U\\
   LOCK850.077B &  3.74 &  0.32 &  0.34 &   5.01 &   4 & LMC &  500 &    1.6 &    7.5& 0.69 & U\\
    LOCK850.078 &  3.38 &  0.00 &  2.64 &   0.57 &   1 & SMC &   50 &    1.4 &    50 & 0.02\\
    LOCK850.079 &  1.96 &  0.24 &  0.22 &   2.50 &   7 &  MW &  600 &    1.2 &   22.5& 0.57\\
    LOCK850.081 &  3.18 &  1.04 &  0.92 &   0.83 &   5 & SMC &  400 &    2.0 &   42.5& 0.84 & I\\
    LOCK850.083 &  0.44 &  0.08 &  0.06 &   1.89 &   7 & LMC &  600 &    1.4 &     0 & 0.00\\
    LOCK850.087 &  2.54 &  0.82 &  0.82 &   0.50 &   5 & SMC &  300 &    1.4 &     0 & 0.57\\
    LOCK850.100 &  3.66 &  3.40 &  2.60 &   1.85 &   1 & SMC &  200 &    1.6 &    55 & 0.08\\
\hline
\end{tabular}
\tablefoot {All parameters are dimensionless except the age which is in Myr. In the final column, 
``C'' notes possibly contaminated flux at $15~\mu$m, 
``D'' notes a depreciated identification, 
``I'' insufficient data to determine the AGN bolometric fraction, 
``U'' an uncertain identification, 
and ``X'' a far-infrared excess.}
\end{table}