\begin{table}%t1
\caption{\label{table:summary}Time-averaged properties of the mass distributions for solenoidal and compressive forcing calculated with the physical scalings applied in PN07.}
%\centering
\par
\begin{tabular}{ccccccccc}        
\hline   \hline  \noalign{\smallskip}            
\multicolumn{9}{c}{Solenoidal forcing, $\zeta=1.0$}\\
\hline
Grid points	 & $\left<\overline{m}\right>\ [{M_{\sun}}]$ & $\left<\sigma_{m}\right>\ [{M_{\sun}}]$ 	 	& $\left<n_{{\rm tot}}\right>$ & $\left<m_{{\rm cores}}/ m_{{\rm tot}}\right>\ [\%]$ & $x_{{\rm LS}}$  & $\left<x_{{\rm MLE}}\right>$ & $\left<m_{{\rm min}}\right>\ [{M_{\sun}}]$ & $\left<p\right>$\\  \hline                         
   ${\rm 256}^3$ 	& $4.04\pm0.18$ & $7.00\pm0.69$	  & $1540\pm57$ & $5.1\pm0.2$&$2.1\pm0.5$ &  $1.8\pm0.5$ & $9.8\pm4.9$&  $0.03\pm0.07$	\\      
   ${\rm 512}^3$ 	& $1.83\pm0.04$	& $2.26\pm0.10$   &$3918\pm103$ &$5.9\pm0.2$ & $3.1\pm0.3$	 & $2.7\pm0.7$ & $6.1\pm2.6$& $0.06\pm0.09$		\\
   ${\rm 1024}^3$	& $1.08\pm0.02$	& $1.05\pm0.04$   &$7082\pm219$ & $6.3\pm0.2$&$3.1 \pm0.2$  &$3.2\pm0.7$ & $3.5\pm0.9$&  $0.21\pm0.26$\\ 
\hline                              
\multicolumn{9}{c}{compressive forcing, $\zeta=0.0$}\\
\hline
   ${\rm 256}^3$ 	& $9.7\pm8.0$ 	& $34.36\pm29.67$&$590\pm57$ & $4.0\pm0.7$&$1.0\pm0.3$ &$1.1\pm0.3$	& $9.7\pm8.0$	& $0.05\pm0.07$	\\
   ${\rm 512}^3$ 	& $2.41\pm0.19$	& $5.54\pm1.48$	&$1859\pm138$ & $3.7\pm0.3$&$1.6\pm0.2$ & $1.6\pm0.3$ & $5.2\pm2.7$ & $0.18\pm0.22$	\\
   ${\rm 1024}^3$	& $0.98\pm0.04$ & $1.44\pm0.21$	& $4985\pm429$& $4.0\pm0.3$&$2.1\pm0.2$ & $2.2\pm0.3$	& $2.7\pm0.8$	& $0.23\pm0.21$ \\ 
\hline                                    
\end{tabular}\vspace*{1.3mm}
\end{table}