\begin{table}%t2
         \caption{\label{table:vlbi}The component parameters of the VLBI images at 5~GHz.}
%\centerline
{\small
\begin{tabular}{ccccccccccccc}
          \hline
           \hline
            \noalign{\smallskip}
1  &2      & 3       &4        &  5       &   6  & 7      & 8  & 9   & 10  & 11 & 12     \\
Name   &$T$& rms & $S_{\rm vlbi}$ & Comp.   &  $S_{\rm p}$  &  $S_{\rm int}$  & $\theta_{1}\times\theta_{2}$ & PA      & $D$       & PA  & $T_{\rm b}$  \\
\& Class &(min)& (mJy/b) & (mJy)&          &   (mJy/b)   &   (mJy)       &     (mas$\times$mas)           & ($^\circ$)  & (mas)    & ($^\circ$) &($\times10^{8}$~K)\\
            \hline
            \noalign{\smallskip}
J0210+0419 &50&0.8&243 &A       &94      &141     & 3.2 $\times$ 2.0             &1.4       &0              &                   &11.8         \\
CSO        &   &  &   &B1      &28      &65      & 4.2 $\times$ 3.8             &176      &71.4 $\pm$ 0.1 & $-152.7 \pm 0.1$    &2.2          \\
           &   &  &  &B2      &22      &63      & 6.3 $\times$ 2.9             &38       &67.1 $\pm$ 0.1 &$-152.7 \pm 0.1$    &1.8  \\
J0323+0534 &149&0.2&135 &A1      &19      &19       & 5.0 $\times$ 1.0             &83       &0              &                   &0.3      \\
CSOc       &   &   &  &A2      &42      &109     & 16.8 $\times$ 5.1            &59        &5.2 $\pm$ 0.1  &42.9 $\pm$ 0.1    &0.3  \\
           &   &   &  &A3      &8       &16       & 12.9 $\times$ 3.8            &63        &22.8 $\pm$ 0.1 &57.4 $\pm$ 0.1    & 0.1       \\
J0433$-$0229&162&0.8& 449 &A1      &270     &388      & 5.0 $\times$ 3.8    &161       &0          &             &6.7          \\
 CSOc/cj    &   &   &    &A2      &30      &35       & 3.7 $\times$ 1.3             &157       &13.0 $\pm$ 0.1 &166.4 $\pm$ 0.1   &2.4   \\
            &   &   &   &B       &9       &15       & 7.9 $\times$ 3.2             &156      &52.6 $\pm$ 0.1 &154.8 $\pm$ 0.1    &0.2     \\
J0913+1454 &108&0.2& 253  &A1      &24      &59       & 2.9 $\times$ 1.5            &105       &0              &                   &4.0    \\
  CSOc     &&  & &A2      &11      &37       & 3.7 $\times$ 2.6             &116       &1.4 $\pm$ 0.1  &$-81.8 \pm 0.4$   &1.0        \\
           &&  & &A3      &3       &5        & 3.5 $\times$ 1.6             &169       &5.5 $\pm$ 0.1  &$-77.0 \pm 0.4$   &0.3       \\
           &&  & &A4      &17      &41       & 2.7 $\times$ 2.3             &72        &10.6 $\pm$ 0.1 &$-85.5 \pm 0.1$   &2.0        \\
           &&  & &A5      &16      &41       & 3.0 $\times$ 2.0             &94        &11.5 $\pm$ 0.1 &$-86.9 \pm 0.1$   &2.0      \\
           &&  & &A6      &11      &21       & 2.2 $\times$ 1.6             &69         &5.6 $\pm$ 0.1  &91.6 $\pm$ 0.1   &2.0   \\
           &&  & &A7      &3       &9        & 4.2 $\times$ 3.0             &25         &6.6 $\pm$ 0.1  &91.7 $\pm$ 0.4   &0.2       \\
           &&  & &A8      &2       &3        & 2.8 $\times$ 1.1             &37        &11.8 $\pm$ 0.1 &88.8 $\pm$ 0.3    &0.3     \\
           &&  & &B       &19      &47       & 3.0 $\times$ 0.6             &117        &54.1 $\pm$ 0.1 &71.7 $\pm$ 0.1   &8.0       \\
J1057+0012 &84&0.3& 316  &A       &183     &289      & 3.1 $\times$ 1.4         &36        &0          &            & 23.0    \\
    cj     &  &  & &        &        &         &                              &           &              &                  &            \\
J1109+1043 &90&0.2& 386  &A       &173     &278      & 4.4 $\times$ 1.7             &58        &0           &                     & 12.0    \\
  CSOc     &  &   & &B       &55      &88       & 4.3 $\times$ 1.7             &65        &46.3 $\pm$ 0.1 &103.3 $\pm$ 0.1   &4.0     \\
J1135$-$0021&60&0.7&358  &A1      &134     &185      & 3.3 $\times$ 2.2             &171       &0            &                    &11.0       \\
   CSO      && & &A2      &29      &69       & 7.4 $\times$ 2.4             &135       &3.3 $\pm$ 0.5  &165.0 $\pm$ 4.2   &1.6   \\
            && & &A3      &9       &27       & 10.5 $\times$ 2.2            &41        &14.5 $\pm$ 1.9 &165.5 $\pm$ 3.5   &0.5    \\
            && & &B1      &44      &79       & 6.0 $\times$ 2.4             &176       &94.6 $\pm$ 0.3 &163.3 $\pm$ 0.1   &2.3        \\
            && & &B2      &35      &91       & 8.8 $\times$ 3.0             &158       &91.4 $\pm$ 0.5 &162.7 $\pm$ 0.1   &1.5    \\
            && & &B3      &19      &69       & 13.6 $\times$ 2.6            &154       &86.6 $\pm$ 1.2 &163.6 $\pm$ 0.2   &0.8   \\
J1203+0414 &48&0.2& 461  &A1      &260     &396      & 2.5 $\times$ 1.1             &118       &0       &                         & 68.4  \\
  cj       &&  & &A2      &25      &56       & 4.5 $\times$ 1.3             &126       &4.3 $\pm$ 0.1  &119.5 $\pm$ 0.1   &2.0   \\
           &&  & &B       &11      &15       & 1.9 $\times$ 1.1             &94        &14.6 $\pm$ 0.1 &101.4 $\pm$ 0.1   &3.0  \\
           &&  & &C       &8       &12       & 2.8 $\times$ 0.4             &111       &63.3 $\pm$ 0.1 &104.4 $\pm$ 0.1   &5.0    \\
J1352+0232 &45&0.2& 202  &A1      &90      &106      & 3.6 $\times$ 1.7             &95        &0      &      &    6.0    \\
  CSOc     &&&    &A2      &57      &68       & 4.3 $\times$ 1.7             &59         &7.1 $\pm$ 0.1 &$-133.6 \pm 0.1$   &3.0    \\
           &&  & &B       &10      &13       & 4.9 $\times$ 1.2             &168       &170.1 $\pm$ 0.1 &$-112.6 \pm 0.1$  & 0.8  \\
J1352+1107 &54&0.5& 102  &A       &29      &77       & 9.2 $\times$ 3.7             &138       &0       &        &1.0 \\
  cx       && &  &B       &13      &60       & 14.3 $\times$ 5.4            &39        &5.2 $\pm$ 0.1 &56.4 $\pm$ 0.1      & 0.3    \\
           && &  &C       &15      &46       & 12.4 $\times$ 2.8            &20        &4.8 $\pm$ 0.1 &$-39.7 \pm 0.1$     &0.5   \\
J1600$-0037$&103&0.2& 169 &A       &70      &83       & 2.5 $\times$ 2.2             &130       &0      &                           &   \\
 cj         &&&  &B1      &29      &57       & 10.0 $\times$ 1.0            &69         &31.8 $\pm$ 0.1 &84.6 $\pm$ 0.1    &    \\
            && & &B2      &21      &46       & 10.9 $\times$ 1.2            &80        &25.2 $\pm$ 0.1 &87.5 $\pm$ 0.1     &    \\
            && & &C       &4       &4        & 1.8 $\times$ 1.1             &72         &50.8 $\pm$ 0.1 &77.8 $\pm$ 0.1    &  \\
J2058+0540 &47&0.4& 220  &A1      &104     &124      & 4.5 $\times$ 1.0             &9.3       &0       &                          & 14.0   \\
   CSO     &&  & &A2      &8.2     &13       & 7.7 $\times$ 2.1             &177       &15.5 $\pm$ 0.1 &$-175.0 \pm 0.2$   & 0.4     \\
           &&  & &B       &42      &68       & 8.3 $\times$ 2.4             &172       &132.6 $\pm$ 0.1&171.9 $\pm$ 0.1    & 2.0   \\
\hline
\end{tabular}}
\tablefoot{The columns provide: (1) source name and classification (CSOc: CSO candidate, cj: core-jet, cx: complex); (2) total observing time per source in minutes; (3) noise level per beam in 5~GHz VLBI image; (4) total VLBI flux density; (5) component identification labelled to Paper~I; (6), (7) peak and integral intensity of a fitted Gaussian component at 5~GHz with the AIPS task JMFIT; (8), (9) major/minor axes and position angle of the component at 5~GHz; (10), (11) distance and position angle relative to the first component; and (12) brightness temperature of the component.}\vspace*{2.4mm}
\end{table}