\begin{table}%T7
\caption{\label{table:openingangle}Opening angles of TANAMI sources.}
\small%%\centering

\par
\begin{tabular}{rrrrrrc}
\hline\hline\noalign{\smallskip}
 {Source} & {Class} &  $r$\tablefootmark{1}  & $\theta$\tablefootmark{2}  & {Component size} & {Opening angle} & {Limit?\tablefootmark{3}} \\
{} & {} & {(mas)}  & {(degrees)} & {(mas)} & {(degrees)} & {}
\\
\hline
0047$-$579 & Q & 2.11 & $-$13.0 & 0.26 & 7.2 & Y \\
0208$-$512 & B & 2.93 & 24.3 & 1.88 & 35.6 & N\\
0438$-$436 & Q & 6.54 & $-$44.8 & 1.36 & 11.9 & N \\
0506$-$612 & Q & 3.02 & $-$46.1 & 0.19 & 3.7 & Y \\
0521$-$365 & B & 3.04 & $-$37.2 & 0.36 & 6.9 & N \\
0537$-$441 & Q & 2.57 & 57.2 & 1.41 & 30.9 & N \\
0637$-$752 & Q & 6.08 & 1.5 & 0.42 & 4.0 & Y \\
1104$-$445 & Q & 3.12 & 27.2 & 2.14 & 38.2 & N \\
1144$-$379 & Q & 1.02 & $-$54.3 & 0.65 & 36.4 & N \\
1257$-$326 & Q & 2.8 & $-$36.4 & 1.51 & 30.7 & N \\
1313$-$333 & Q & 3.74 & $-$7.5 & 2.45 & 36.3 & N \\
1323$-$526 & U & 3.26 & 83.2 & 0.41 & 7.3 & N \\
1424$-$418 & Q & 0.98 & 42.5 & 0.87 & 47.9 & N \\
1454$-$354 & Q & 1.77 & 2.6 & 0.87 & 27.5 & N \\
1610$-$771 & Q & 2.16 & $-$48.1 & 0.40 & 10.7 & N \\
1714$-$336 & B & 13.61 & 32.7 & 4.73 & 19.7 & N \\
1716$-$771 & U & 2.3 & 49.8 & 0.30 & 7.4 & Y \\
1759$-$396 & Q & 2.61 & $-$74.6 & 1.67 & 36.2 & N \\
1804$-$502 & Q & 2.29 & 54.1 & 0.96 &23.9 & N \\
1933$-$400 & Q & 2.39 & $-$51.0 & 0.31 & 7.6 & Y \\
1954$-$388 & Q & 1.55 & $-$44.1 & 0.45 & 16.5 & N \\
2005$-$489 & B & 1.52 & 31.8 & 1.18 & 42.4 & N \\
2052$-$474 & Q & 1.91 & $-$31.0 & 0.27 & 8.0 & N \\
2106$-$413 & Q & 3.1 & 1.7 & 0.47 & 8.6 & Y \\
2149$-$306 & Q & 2.49 & $-$28.1 & 0.26 & 6.0 & Y \\
2155$-$304 & B & 2.72 & $-$56.2 & 1.74 & 35.4 & N \\
2204$-$540 & Q & 2.14 & 64.6 & 0.30 & 8.0 & N \\
2326$-$477 & Q & 3.47 & $-$11.0 & 0.30 & 5.0 & Y \\
2355$-$534 & Q & 3.88 & 37.9 & 0.49 & 7.3 & N \\
\hline
\end{tabular}
\tablefoot{\tablefoottext{1}{Radial distance between core and fitted component.} %\\\\
\tablefoottext{2}{Angle between core and fitted component.} %\\\\
\tablefoottext{3}{Flag indicating whether the innermost jet component is unresolved, resulting in an upper limit on the opening angle. Y = yes, N = no.}}\vspace*{3mm}
\end{table}