\begin{table}%t6
\par
\caption {\label{tab:noise_performances}Receiver noise properties: $1/f$ knee frequency, slope, and $r$~factor. } 
%\centering
                          % used for centering table
\begin{tabular}{l l r r r r}        % centered columns (4 columns)
\hline\hline                 % inserts double horizontal lines
\noalign{\smallskip}
 & & \multicolumn{4}{c}{1\sc{/{\it f} spectrum, r factor, and $\beta$}}\\
 & & M-00 & M-01 & S-10 & S-11 \\    % table heading 
\hline                        % inserts single horizontal line
{\tt RCA18}  
& $f_{\rm k}$ & 92 & 92 & 140 & 190\\
& $\alpha$& --1.62 & --1.71 & --1.49 & --1.71 \\
& $r$    & 1.17& 1.17& 1.17& 1.16 \\
& $\beta$  & 9.57   & 10.30  &  8.53 & 10.78\\
{\tt RCA19}  
& $f_{\rm k}$  & 130 &	96&144	&143 \\
& $\alpha$&  --1.75 & --1.93& --1.80 & --1.85\\
& $r$    & 1.12& 1.12&  1.14& 1.13  \\
& $\beta$  &  8.90  &  9.10 & 9.00  & 11.06\\
{\tt RCA20}  
& $f_{\rm k}$  & 55.7&	63.7&	119.3& 98.5\\
& $\alpha$&--1.63 &--1.48 &--1.36 & --1.32\\
& $r$    & 1.03& 1.02& 1.03& 1.04 \\
& $\beta$  & 10.74   & 9.46  & 10.86  & 10.48\\
{\tt RCA21}  
& $f_{\rm k}$  & 109&	85&	109& 97\\
& $\alpha$& --1.59& --1.90&--1.61 &--1.17 \\
& $r$    & 1.21&1.21 &1.18 &1.18  \\
& $\beta$  &10.02    &10.08   & 9.79  &8.79 \\
{\tt RCA22}  
& $f_{\rm k}$  &116 &108	&80	& 113\\
& $\alpha$& --1.59& --1.90& --1.61& --1.65\\
& $r$    & 1.21& 1.21& 1.18& 1.18 \\
& $\beta$  &   10.02 &10.8   & 9.79  &8.79 \\
{\tt RCA23}  
& $f_{\rm k}$  & 97&89	&101	&109 \\
& $\alpha$& --1.41& --1.92& --1.90& --1.83\\
& $r$    & 1.07&1.07 &1.08 &1.08  \\
& $\beta$  &  11.31  & 13.02  & 11.05  & 11.89\\
{\tt RCA24}\tablefootmark{a}
& $f_{\rm k}$  &13.9 &10.2&9.7& 13.3\\
& $\alpha$&--1.13& --1.26&--1.15& --1.18\\
& $r$    &0.991&0.974&0.971& 0.962\\
& $\beta$  &   6.13 &  4.12 &  5.21 & 6.59\\
{\tt RCA25}\tablefootmark{b} 
& $f_{\rm k}$  &18.0&	21.9&	9.6& 4.7\\
& $\alpha$& --1.12&--1.28&1.04&--0.89\\
& $r$    &1.0289& 1.059& --0.859&   1.041\\
& $\beta$  & 6.87   & 6.88  & 4.96  & 6.82\\
{\tt RCA26}$^{\rm c}$
& $f_{\rm k}$  &21.0&23.2&15.4&23.1\\
& $\alpha$&--1.02&--0.72&--0.67& --0.81\\
& $r$    &1.085&1.061&1.131& 1.119\\
& $\beta$  &  5.67  & 5.52  &   5.01& 7.40 \\
{\tt RCA27}\tablefootmark{d}
& $f_{\rm k}$  & 6.7&10.1&	24.9&31.1\\
& $\alpha$&--1.02&--1.19&--1.39& --0.90\\
& $r$    &1.012&1.004&1.093& 1.075\\
& $\beta$  & 7.77   & 7.70  & 8.73  & 7.18\\
{\tt RCA28}\tablefootmark{e} 
& $f_{\rm k}$  &19.9&19.4&40.7&41.1\\
& $\alpha$& --1.39& --1.20& --1.57&--1.60\\
& $r$    &1.058 &1.050&0.955& 0.939\\
& $\beta$  &  7.91  & 7.94  &8.78   & 8.23\\
\hline                                   
\end{tabular}
\tablefoot {Data were taken setting the temperature of the loads at the lowest possible values. The 70 GHz $1/f$ knee frequencies are dominated by the thermal instabilities of the cryochamber.
\tablefoottext{a}{$T_{\rm ref}=8.5$~K; $T_{\rm sky}=8.5$~K.}\\
                           \tablefoottext{b}{$T_{\rm ref}=8.0$~K; $T_{\rm sky}=10.5$~K.}
	       \tablefoottext{c}{$T_{\rm ref}=8.0$~K; $T_{\rm sky}=13.0$~K.}
 	       \tablefoottext{d}{$T_{\rm ref}=9.5$~K; $T_{\rm sky}=12.8$~K.}
 	       \tablefoottext{e}{$T_{\rm ref}=8.6$~K; $T_{\rm sky}=8.5$~K.}}
\end{table}