\begin{table}%t3
\caption{\label{JMLTab:Spectral}Estimated average redundancy of observations in one year of
operation for $2^\prime$~$\times$ $2^\prime$~pixels. The average observation time is per bolometer.}
%\centering
\par
\begin{tabular}{l*{9}{c}}
\hline \hline \noalign{\smallskip}
Frequency (GHz) and mode  & 100P & 143P & 143 & 217P & 217 & 353P & 353 & 545 & 857 \\
\hline
Average obs time (s/sample) & 2.9 & 1.8 & 1.8 & 0.85 & 0.85 & 0.85 & 0.85 & 0.85 & 0.85 \\
Average redundancy (1~year)  & 1380 & 850 & 1250 & 400 & 600 & 400 & 600 & 600 & 600 \\
Max. redundancy (1~year) & 12~000 & 7700 & 12~000 & 3700 & 5600 & 3700 & 5600 & 5600 & 5600 \\
Min. redundancy (1year) & 700 & 420 & 630 & 200 & 300 & 200 & 300 & 300 & 300 \\
\hline
\end{tabular}
\end{table}