\begin{table}%t4
\caption{\label{JMLTab:Tau}The time response of each bolometer family is given by the average cut-off frequency of transfer functions. }
%\centering
\par
\begin{tabular}{l*{9}{c}}
\hline
\hline \noalign{\smallskip}
Channel  & 100P & 143P &143 &217P &217 & 353P & 353 & 545 & 857 \\
\hline
Beam size (\arcmin) &9.6 &6.9 &7.1 &4.6 &4.6 &4.6 &4.7 &4.7 & 4.3 \\
Average cut-off frequency @3dB (Hz) &14 &29 &28 &26 &55 &27 &52 &74 & 72 \\
\hline
\end{tabular}
 \tablefoot{The suffix~P stands for polarisation sensitive bolometers.}
\end{table}