\begin{table}%t1
\caption{\label{32890_tab}Parameters for the fit to CoRoT 102732890.}
%\centering
\par
\begin{tabular}{cccccc}
\hline\hline\noalign{\smallskip}
Frequency & Linewidth  & Height  &  $H/B$  & Amplitude & Lifetime \\
 $\mu$Hz  &  $\mu$Hz & 10$^5$ ppm$^2~\mu$Hz$^{-1}$ &  & ppm & days\\
\hline
20.96 $\pm$ 0.033 & 0.026 $\pm$ 0.003 & 0.5 $\pm$ 0.1 & 9.7 & 64 $\pm$ 26 & $>$100\\
(22.2 $\pm$ 0.2 & 0.27 $\pm$ 0.04 & 0.20 $\pm$ 0.02 & 11.6 & 130 $\pm$ 33 & $\rm 10.0^{+3.6}_{-2.4}$)\\
$[$22.0 $\pm$ 0.1 & 0.040 $\pm$ 0.004 & 0.37 $\pm$ 0.05 & 11.4 & 69 $\pm$ 17 & $>$100$]$\\
$[$22.3 $\pm$ 0.1 & 0.16 $\pm$ 0.03 & 0.22 $\pm$ 0.04 & 11.7 & 103 $\pm$ 30 & $\rm 28.3^{+30.0}_{-8.7}$$]$\\
24.08 $\pm$ 0.06 & 0.07  $\pm$ 0.01 & 0.6 $\pm$ 0.1 & 19.5 & 107 $\pm$ 38 & $>$100\\
25.14 $\pm$ 0.03 & 0.036 $\pm$ 0.003  & 0.7 $\pm$ 0.1 & 30.9 & 87 $\pm$ 27 & $>$100\\
25.62 $\pm$ 0.04 & 0.050 $\pm$ 0.002 & 0.93 $\pm$ 0.05 & 30.8 & 120 $\pm$ 20 & $>$100\\
27.27 $\pm$ 0.07 & 0.21 $\pm$ 0.01 & 0.3 $\pm$ 0.1 & 20.3 & 136 $\pm$ 83 & $\rm 16.1^{+1.6}_{-1.4}$\\
28.7 $\pm$ 0.6 & 0.2 $\pm$ 0.1 & 0.11 $\pm$ 0.05 & 9.9 & 85 $\pm$ 37 & $\rm 17.7^{+82.3}_{-9.6}$\\
30.45 $\pm$ 0.07 & 0.079 $\pm$ 0.005 & 0.14 $\pm$ 0.01 & 8.4 & 59 $\pm$ 11 & $>$100\\
31.6 $\pm$ 0.1 & 0.084 $\pm$ 0.008 & 0.22 $\pm$ 0.03 & 14.1 & 76 $\pm$ 18 & $>$100\\
\hline
\end{tabular}
\tablefoot{ The result between ``()'' is the oscillation mode at $\sim$22~$\mu$Hz in the fit with nine frequencies, while the results for the interpretation of two oscillation modes at $\sim$22~$\mu$Hz are indicated in square brackets. The frequencies, linewidth and height are fitted parameters, the height-to-background ratio ($H/B$) is measured as the observed height of the oscillation mode in the power spectrum over the fitted background. The amplitudes and ``unbiased'' lifetimes are derived from the fitted parameters as described in the text.}
\end{table}