\begin{table}%t3
%%\centering
\par
\caption{Summary of the instrumental parameters assumed for the performance simulation of ALADDIN.
The throughput and emissivity are directly computed from the baseline instrumental design, which is
based on a simplified version of the GENIE instrument. \label{tab:instruparam}}
\begin{tabular}[h]{cc}
\hline \hline\multicolumn{2}{c}{Instrumental parameters}
\\ \hline Baselines & $4{-}30$~m
\\        Telescope diameter & 1~m
\\        Number of warm optics & 5
\\        Warm optics temperature & 230~K
\\        Warm throughput & 80\%
\\        Warm emissivity & 20\%
\\        Number of cold optics & 15
\\        Cryogenic temperature & 77~K
\\        Cold throughput & 10\%
\\        Science waveband & $3.1{-}4.1$~$\mu$m ($L$)
\\        Fringe sensing waveband & $2.0{-}2.4$~$\mu$m ($K$)
\\        Tip-tilt sensing waveband & $1.15{-}1.3$~$\mu$m ($J$)
\\ \hline
\end{tabular}
\end{table}